From a5b709a81ad9a5e2e6e4be6a696711ad7f35ad57 Mon Sep 17 00:00:00 2001
From: Icenowy Zheng <icenowy@aosc.io>
Date: Thu, 9 Feb 2017 00:18:56 +0800
Subject: [PATCH 001/146] arm64: allwinner: a64: enable Wi-Fi for Pine64

The Wi-Fi modules of Pine64 is powered via DLDO4 and ELDO1 (the latter
one provides I/O voltage).

Add device node for it.

Signed-off-by: Icenowy Zheng <icenowy@aosc.io>
---
 .../boot/dts/allwinner/sun50i-a64-pine64.dts     | 16 ++++++++++++++++
 1 file changed, 16 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pine64.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-pine64.dts
index 1b9b92e541d2..d06b5b88f60e 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pine64.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pine64.dts
@@ -62,6 +62,11 @@
 	chosen {
 		stdout-path = "serial0:115200n8";
 	};
+
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		reset-gpios = <&r_pio 0 2 GPIO_ACTIVE_LOW>; /* PL2 */
+	};
 };
 
 &ehci0 {
@@ -109,6 +114,17 @@
 	status = "okay";
 };
 
+&mmc1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc1_pins>;
+	vmmc-supply = <&reg_dldo4>;
+	vqmmc-supply = <&reg_eldo1>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	non-removable;
+	bus-width = <4>;
+	status = "okay";
+};
+
 &ohci0 {
 	status = "okay";
 };
-- 
2.17.1

