diff --git a/arch/arm64/boot/dts/allwinner/Makefile b/arch/arm64/boot/dts/allwinner/Makefile
index 3040c3074..712e1cf5f
--- a/arch/arm64/boot/dts/allwinner/Makefile
+++ b/arch/arm64/boot/dts/allwinner/Makefile
@@ -1,5 +1,6 @@
 # SPDX-License-Identifier: GPL-2.0
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-bananapi-m64.dtb
+dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h6-orangepi-one-plus.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-nanopi-a64.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-olinuxino.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-orangepi-win.dtb
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-one-plus.dts b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-one-plus.dts
new file mode 100644
index 000000000..385015396
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-one-plus.dts
@@ -0,0 +1,254 @@
+// SPDX-License-Identifier: (GPL-2.0+ or MIT)
+/*
+ * Copyright (c) 2018 Armbian
+ */
+
+/dts-v1/;
+
+#include "sun50i-h6.dtsi"
+
+#include <dt-bindings/gpio/gpio.h>
+
+/ {
+	model = "Orange Pi One+";
+	compatible = "xunlong,orangepi-one-plus", "allwinner,sun50i-h6";
+
+	aliases {
+		serial0 = &uart0;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		pwr {
+			label = "orangepi:red:pwr";
+			gpios = <&r_pio 0 4 GPIO_ACTIVE_HIGH>;
+			default-state = "on";
+		};
+
+		status {
+			label = "orangepi:green:status";
+			gpios = <&r_pio 0 7 GPIO_ACTIVE_HIGH>;
+		};
+	};
+
+	reg_gmac_3v3: gmac-3v3 {
+                compatible = "regulator-fixed";
+                regulator-name = "vcc-gmac-3v3";
+                regulator-min-microvolt = <3300000>;
+                regulator-max-microvolt = <3300000>;
+                startup-delay-us = <100000>;
+                enable-active-high;
+                gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>; /* PD6 */
+                vin-supply = <&reg_aldo2>;
+        };
+
+	reg_vcc3v3: vcc3v3 {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+	};
+
+	reg_vcc1v8: vcc1v8 {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc1v8";
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <1800000>;
+	};
+
+	reg_usb_vbus: vbus {
+		compatible = "regulator-fixed";
+		regulator-name = "usb-vbus";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		startup-delay-us = <100000>;
+		gpio = <&r_pio 0 5 GPIO_ACTIVE_HIGH>;
+		enable-active-high;
+	};
+};
+
+&cpu0 {
+	cpu-supply = <&reg_dcdca>;
+};
+
+&ehci0 {
+	status = "okay";
+};
+
+&ehci3 {
+	status = "okay";
+};
+
+
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&ext_rgmii_pins>;
+	phy-mode = "rgmii";
+	phy-handle = <&ext_rgmii_phy>;
+	phy-supply = <&reg_gmac_3v3>;
+	allwinner,rx-delay-ps = <200>;
+	allwinner,tx-delay-ps = <200>;
+	status = "okay";
+};
+
+&dwc3 {
+	status = "okay";
+};
+
+&mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
+};
+
+&mmc0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc0_pins>;
+	vmmc-supply = <&reg_vcc3v3>;
+	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>;
+	status = "okay";
+};
+
+&ohci0 {
+	status = "okay";
+};
+
+&ohci3 {
+	status = "okay";
+};
+
+&r_i2c {
+	status = "okay";
+
+	axp805: pmic@36 {
+		compatible = "x-powers,axp805", "x-powers,axp806";
+		reg = <0x36>;
+		interrupt-parent = <&r_intc>;
+		interrupts = <0 IRQ_TYPE_LEVEL_LOW>;
+		interrupt-controller;
+		#interrupt-cells = <1>;
+		x-powers,master-mode;
+
+		regulators {
+			reg_aldo1: aldo1 {
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-pl";
+			};
+
+			reg_aldo2: aldo2 {
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-ac200";
+			};
+
+			reg_aldo3: aldo3 {
+				/* This regulator is connected with CLDO1 */
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-3v3-1";
+			};
+
+			reg_bldo1: bldo1 {
+				regulator-always-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "vcc-ddr-bias-pll";
+			};
+
+			reg_bldo2: bldo2 {
+				regulator-always-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "vcc-efuse-emmc-pcie-hdmi";
+			};
+
+			reg_bldo3: bldo3 {
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "vcc-wifi-io";
+			};
+
+			bldo4 {
+				/* unused */
+			};
+
+			reg_cldo1: cldo1 {
+				/* This regulator is connected with ALDO3 */
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-3v3-2";
+			};
+
+			reg_cldo2: cldo2 {
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-wifi-1";
+			};
+
+			reg_cldo3: cldo3 {
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-wifi-2";
+ 			};
+
+			reg_dcdca: dcdca {
+				regulator-always-on;
+				regulator-min-microvolt = <810000>;
+				regulator-max-microvolt = <1160000>;
+				regulator-name = "vdd-cpu";
+			};
+
+			reg_dcdcc: dcdcc {
+				regulator-always-on;
+				regulator-min-microvolt = <810000>;
+				regulator-max-microvolt = <1080000>;
+				regulator-name = "vdd-gpu";
+			};
+
+			reg_dcdcd: dcdcd {
+				regulator-always-on;
+				regulator-min-microvolt = <960000>;
+				regulator-max-microvolt = <960000>;
+				regulator-name = "vdd-sys";
+			};
+
+			reg_dcdce: dcdce {
+				regulator-always-on;
+				regulator-min-microvolt = <1400000>;
+				regulator-max-microvolt = <1400000>;
+				regulator-name = "vcc-dram";
+			};
+
+			sw {
+				/* unused */
+			};
+		};
+	};
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_ph_pins>;
+	status = "okay";
+};
+
+&usb2otg {
+	dr_mode = "host";
+	status = "okay";
+};
+
+&usb2phy {
+	usb0_vbus-supply = <&reg_usb_vbus>;
+	usb1_vbus-supply = <&reg_usb_vbus>;
+	status = "okay";
+};
diff --git a/arch/arm64/boot/dts/allwinner/Makefile b/arch/arm64/boot/dts/allwinner/Makefile
index a9797d233..4972f2901
--- a/arch/arm64/boot/dts/allwinner/Makefile
+++ b/arch/arm64/boot/dts/allwinner/Makefile
@@ -1,6 +1,7 @@
 # SPDX-License-Identifier: GPL-2.0
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-bananapi-m64.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h6-orangepi-one-plus.dtb
+dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h6-orangepi-lite2.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-nanopi-a64.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-olinuxino.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-orangepi-win.dtb
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-lite2.dts b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-lite2.dts
new file mode 100644
index 000000000..b9aff606e
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6-orangepi-lite2.dts
@@ -0,0 +1,275 @@
+// SPDX-License-Identifier: (GPL-2.0+ or MIT)
+/*
+ * Copyright (c) 2017 Icenowy Zheng <icenowy@aosc.io>
+ */
+
+/dts-v1/;
+
+#include "sun50i-h6.dtsi"
+
+#include <dt-bindings/gpio/gpio.h>
+
+/ {
+	model = "Orange Pi Lite 2";
+	compatible = "pine64,pine-h64", "allwinner,sun50i-h6";
+
+	aliases {
+		serial0 = &uart0;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		pwr {
+			label = "orangepi:red:pwr";
+			gpios = <&r_pio 0 4 GPIO_ACTIVE_HIGH>;
+			default-state = "on";
+		};
+
+		status {
+			label = "orangepi:green:status";
+			gpios = <&r_pio 0 7 GPIO_ACTIVE_HIGH>;
+		};
+	};
+
+	reg_vcc3v3: vcc3v3 {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+	};
+
+	reg_vcc1v8: vcc1v8 {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc1v8";
+		regulator-min-microvolt = <1800000>;
+		regulator-max-microvolt = <1800000>;
+	};
+
+	reg_usb_vbus: vbus {
+		compatible = "regulator-fixed";
+		regulator-name = "usb-vbus";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		startup-delay-us = <100000>;
+		gpio = <&r_pio 0 5 GPIO_ACTIVE_HIGH>;
+		enable-active-high;
+	};
+
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		clocks = <&rtc 1>;
+		clock-names = "ext_clock";
+		reset-gpios = <&r_pio 1 3 GPIO_ACTIVE_LOW>; /* PM3 */
+		post-power-on-delay-ms = <200>;
+	};
+};
+
+&cpu0 {
+	cpu-supply = <&reg_dcdca>;
+};
+
+&dwc3 {
+	status = "okay";
+};
+
+&ehci0 {
+	status = "okay";
+};
+
+&ehci3 {
+	status = "okay";
+};
+
+&mmc0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc0_pins>;
+	vmmc-supply = <&reg_vcc3v3>;
+	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>;
+	status = "okay";
+};
+
+&mmc1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc1_pins>;
+	vmmc-supply = <&reg_cldo2>;
+	vqmmc-supply = <&reg_bldo3>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+
+	ap6255: sdio_wifi@1 {
+		reg = <1>;
+		compatible = "brcm,bcm4329-fmac";
+		interrupt-parent = <&r_pio>;
+		interrupts = <1 0 IRQ_TYPE_LEVEL_LOW>;	/* PM0 */
+		interrupt-names = "host-wake";
+	};
+};
+
+&mmc2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc2_pins>;
+	vmmc-supply = <&reg_vcc3v3>;
+	vqmmc-supply = <&reg_bldo3>;
+	non-removable;
+	cap-mmc-hw-reset;
+	status = "disabled";
+};
+
+&ohci0 {
+	status = "okay";
+};
+
+&ohci3 {
+	status = "okay";
+};
+
+&r_i2c {
+	pinctrl-names = "default";
+	pinctrl-0 = <&r_i2c_pins>;
+	status = "okay";
+
+	axp805: pmic@36 {
+		compatible = "x-powers,axp805", "x-powers,axp806";
+		reg = <0x36>;
+		interrupt-parent = <&r_intc>;
+		interrupts = <0 IRQ_TYPE_LEVEL_LOW>;
+		interrupt-controller;
+		#interrupt-cells = <1>;
+		x-powers,self-working-mode;
+
+		regulators {
+			reg_aldo1: aldo1 {
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-pl";
+			};
+
+			reg_aldo2: aldo2 {
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-ac200";
+			};
+
+			reg_aldo3: aldo3 {
+				/* This regulator is connected with CLDO1 */
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-3v3-1";
+			};
+
+			reg_bldo1: bldo1 {
+				regulator-always-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "vcc-ddr-bias-pll";
+			};
+
+			reg_bldo2: bldo2 {
+				regulator-always-on;
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "vcc-efuse-emmc-pcie-hdmi";
+			};
+
+			reg_bldo3: bldo3 {
+				regulator-min-microvolt = <1800000>;
+				regulator-max-microvolt = <1800000>;
+				regulator-name = "vcc-wifi-io";
+			};
+
+			bldo4 {
+				/* unused */
+			};
+
+			reg_cldo1: cldo1 {
+				/* This regulator is connected with ALDO3 */
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-3v3-2";
+			};
+
+			reg_cldo2: cldo2 {
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-wifi-1";
+			};
+
+			reg_cldo3: cldo3 {
+				regulator-always-on;
+				regulator-min-microvolt = <3300000>;
+				regulator-max-microvolt = <3300000>;
+				regulator-name = "vcc-wifi-2";
+			};
+
+			reg_dcdca: dcdca {
+				regulator-always-on;
+				regulator-min-microvolt = <810000>;
+				regulator-max-microvolt = <1160000>;
+				regulator-name = "vdd-cpu";
+			};
+
+			reg_dcdcc: dcdcc {
+				regulator-min-microvolt = <810000>;
+				regulator-max-microvolt = <1080000>;
+				regulator-name = "vdd-gpu";
+			};
+
+			reg_dcdcd: dcdcd {
+				regulator-always-on;
+				regulator-min-microvolt = <960000>;
+				regulator-max-microvolt = <960000>;
+				regulator-name = "vdd-sys";
+			};
+
+			reg_dcdce: dcdce {
+				regulator-always-on;
+				regulator-min-microvolt = <1400000>;
+				regulator-max-microvolt = <1400000>;
+				regulator-name = "vcc-dram";
+			};
+
+			sw {
+				/* unused */
+			};
+		};
+	};
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_ph_pins>;
+	status = "okay";
+};
+
+&uart1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart1_pins>;
+	status = "disabled";
+};
+
+&usb2otg {
+	dr_mode = "host";
+	status = "okay";
+};
+
+&usb2phy {
+	usb0_vbus-supply = <&reg_usb_vbus>;
+	usb3_vbus-supply = <&reg_usb_vbus>;
+	status = "okay";
+};
+
+&usb3phy {
+	phy-supply = <&reg_usb_vbus>;
+	status = "okay";
+};
