From a73c51c6adf95985d02f22670f45bc8d6a84739c Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Tue, 14 Nov 2017 17:17:14 +0100
Subject: [PATCH 60/82] ARM: dts: sun8i-a83t-tbs-a711: Enable thermal sensor

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts b/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
index bc08c3c281c1..ed59185b9105 100644
--- a/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
+++ b/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
@@ -588,6 +588,10 @@
 	};
 };
 
+&ths {
+	status = "okay";
+};
+
 &uart0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart0_pb_pins>;
-- 
2.20.1

