diff --git a/arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts b/arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts
index b3283ae..46a1507 100644
--- a/arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts
+++ b/arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts
@@ -103,6 +103,8 @@
 		compatible = "mmc-pwrseq-simple";
 		pinctrl-names = "default";
 		reset-gpios = <&r_pio 0 7 GPIO_ACTIVE_LOW>; /* PL7 */
+		clocks = <&rtc 1>;
+		clock-names = "ext_clock";
 	};
 };

@@ -215,7 +217,19 @@
 &uart1 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart1_pins>, <&uart1_rts_cts_pins>;
-	status = "okay";
+	uart-has-rtscts;
+	status = "okay";
+
+	bluetooth {
+		compatible = "brcm,bcm43438-bt";
+		clocks = <&rtc 1>;
+		clock-names = "lpo";
+		vbat-supply = <&reg_vcc3v3>;
+		vddio-supply = <&reg_vcc3v3>;
+		device-wakeup-gpios = <&pio 6 13 GPIO_ACTIVE_HIGH>; /* PG13 */
+		host-wakeup-gpios = <&pio 6 11 GPIO_ACTIVE_HIGH>; /* PG11 */
+		shutdown-gpios = <&pio 6 12 GPIO_ACTIVE_HIGH>; /* PG12 */
+	};
 };

 &usb_otg {
