From 08c47cbb508e40e5e404055f77653474d5793e27 Mon Sep 17 00:00:00 2001
From: Vasily Khoruzhick <anarsoul@gmail.com>
Date: Wed, 31 Oct 2018 20:33:22 -0700
Subject: [PATCH 143/146] Bluetooth: btrtl: add support for the RTL8723CS

The Realtek RTL8723CS is SDIO WiFi chip. It also contains a Bluetooth
module which is connected via UART to the host.

It shares lmp subversion with 8703B, so Realtek's userspace
initialization tool (rtk_hciattach) differentiates varieties of RTL8723CS
(CG, VF, XX) with RTL8703B using vendor's command to read chip type.

Also this chip declares support for some features it doesn't support
so add a quirk to indicate that these features are broken.

Signed-off-by: Vasily Khoruzhick <anarsoul@gmail.com>
---
 drivers/bluetooth/btrtl.c  | 128 ++++++++++++++++++++++++++++++++++++-
 drivers/bluetooth/btrtl.h  |  12 ++++
 drivers/bluetooth/hci_h5.c |   4 ++
 3 files changed, 141 insertions(+), 3 deletions(-)

diff --git a/drivers/bluetooth/btrtl.c b/drivers/bluetooth/btrtl.c
index 7f9ea8e4c1b2..f9474e78bcfa 100644
--- a/drivers/bluetooth/btrtl.c
+++ b/drivers/bluetooth/btrtl.c
@@ -27,8 +27,12 @@
 
 #define VERSION "0.1"
 
+#define RTL_CHIP_8723CS_CG	3
+#define RTL_CHIP_8723CS_VF	4
+#define RTL_CHIP_8723CS_XX	5
 #define RTL_EPATCH_SIGNATURE	"Realtech"
 #define RTL_ROM_LMP_3499	0x3499
+#define RTL_ROM_LMP_8703B	0x8703
 #define RTL_ROM_LMP_8723A	0x1200
 #define RTL_ROM_LMP_8723B	0x8723
 #define RTL_ROM_LMP_8821A	0x8821
@@ -40,6 +44,7 @@
 #define IC_MATCH_FL_HCIREV	(1 << 1)
 #define IC_MATCH_FL_HCIVER	(1 << 2)
 #define IC_MATCH_FL_HCIBUS	(1 << 3)
+#define IC_MATCH_FL_CHIP_TYPE	(1 << 4)
 #define IC_INFO(lmps, hcir) \
 	.match_flags = IC_MATCH_FL_LMPSUBV | IC_MATCH_FL_HCIREV, \
 	.lmp_subver = (lmps), \
@@ -51,6 +56,7 @@ struct id_table {
 	__u16 hci_rev;
 	__u8 hci_ver;
 	__u8 hci_bus;
+	__u8 chip_type;
 	bool config_needed;
 	bool has_rom_version;
 	char *fw_name;
@@ -98,6 +104,39 @@ static const struct id_table ic_id_table[] = {
 	  .fw_name  = "rtl_bt/rtl8723b_fw.bin",
 	  .cfg_name = "rtl_bt/rtl8723b_config" },
 
+	/* 8723CS-CG */
+	{ .match_flags = IC_MATCH_FL_LMPSUBV | IC_MATCH_FL_CHIP_TYPE |
+			 IC_MATCH_FL_HCIBUS,
+	  .lmp_subver = RTL_ROM_LMP_8703B,
+	  .chip_type = RTL_CHIP_8723CS_CG,
+	  .hci_bus = HCI_UART,
+	  .config_needed = true,
+	  .has_rom_version = true,
+	  .fw_name  = "rtl_bt/rtl8723cs_cg_fw.bin",
+	  .cfg_name = "rtl_bt/rtl8723cs_cg_config" },
+
+	/* 8723CS-VF */
+	{ .match_flags = IC_MATCH_FL_LMPSUBV | IC_MATCH_FL_CHIP_TYPE |
+			 IC_MATCH_FL_HCIBUS,
+	  .lmp_subver = RTL_ROM_LMP_8703B,
+	  .chip_type = RTL_CHIP_8723CS_VF,
+	  .hci_bus = HCI_UART,
+	  .config_needed = true,
+	  .has_rom_version = true,
+	  .fw_name  = "rtl_bt/rtl8723cs_vf_fw.bin",
+	  .cfg_name = "rtl_bt/rtl8723cs_vf_config" },
+
+	/* 8723CS-XX */
+	{ .match_flags = IC_MATCH_FL_LMPSUBV | IC_MATCH_FL_CHIP_TYPE |
+			 IC_MATCH_FL_HCIBUS,
+	  .lmp_subver = RTL_ROM_LMP_8703B,
+	  .chip_type = RTL_CHIP_8723CS_XX,
+	  .hci_bus = HCI_UART,
+	  .config_needed = true,
+	  .has_rom_version = true,
+	  .fw_name  = "rtl_bt/rtl8723cs_xx_fw.bin",
+	  .cfg_name = "rtl_bt/rtl8723cs_xx_config" },
+
 	/* 8723D */
 	{ IC_INFO(RTL_ROM_LMP_8723B, 0xd),
 	  .config_needed = true,
@@ -147,7 +186,8 @@ static const struct id_table ic_id_table[] = {
 	};
 
 static const struct id_table *btrtl_match_ic(u16 lmp_subver, u16 hci_rev,
-					     u8 hci_ver, u8 hci_bus)
+					     u8 hci_ver, u8 hci_bus,
+					     u8 chip_type)
 {
 	int i;
 
@@ -164,6 +204,9 @@ static const struct id_table *btrtl_match_ic(u16 lmp_subver, u16 hci_rev,
 		if ((ic_id_table[i].match_flags & IC_MATCH_FL_HCIBUS) &&
 		    (ic_id_table[i].hci_bus != hci_bus))
 			continue;
+		if ((ic_id_table[i].match_flags & IC_MATCH_FL_CHIP_TYPE) &&
+		    (ic_id_table[i].chip_type != chip_type))
+			continue;
 
 		break;
 	}
@@ -225,6 +268,7 @@ static int rtlbt_parse_firmware(struct hci_dev *hdev,
 		{ RTL_ROM_LMP_8723B, 1 },
 		{ RTL_ROM_LMP_8821A, 2 },
 		{ RTL_ROM_LMP_8761A, 3 },
+		{ RTL_ROM_LMP_8703B, 7 },
 		{ RTL_ROM_LMP_8822B, 8 },
 		{ RTL_ROM_LMP_8723B, 9 },	/* 8723D */
 		{ RTL_ROM_LMP_8821A, 10 },	/* 8821C */
@@ -499,6 +543,48 @@ static struct sk_buff *btrtl_read_local_version(struct hci_dev *hdev)
 	return skb;
 }
 
+static bool rtl_has_chip_type(u16 lmp_subver)
+{
+	switch (lmp_subver) {
+	case RTL_ROM_LMP_8703B:
+		return true;
+	default:
+		break;
+	}
+
+	return  false;
+}
+
+static int rtl_read_chip_type(struct hci_dev *hdev, u8 *type)
+{
+	struct rtl_chip_type_evt *chip_type;
+	struct sk_buff *skb;
+	const unsigned char cmd_buf[] = {0x00, 0x94, 0xa0, 0x00, 0xb0};
+
+	/* Read RTL chip type command */
+	skb = __hci_cmd_sync(hdev, 0xfc61, 5, cmd_buf, HCI_INIT_TIMEOUT);
+	if (IS_ERR(skb)) {
+		rtl_dev_err(hdev, "Read chip type failed (%ld)",
+			    PTR_ERR(skb));
+		return PTR_ERR(skb);
+	}
+
+	if (skb->len != sizeof(*chip_type)) {
+		rtl_dev_err(hdev, "RTL chip type event length mismatch");
+		kfree_skb(skb);
+		return -EIO;
+	}
+
+	chip_type = (struct rtl_chip_type_evt *)skb->data;
+	rtl_dev_info(hdev, "chip_type status=%x type=%x",
+		     chip_type->status, chip_type->type);
+
+	*type = chip_type->type & 0x0f;
+
+	kfree_skb(skb);
+	return 0;
+}
+
 void btrtl_free(struct btrtl_device_info *btrtl_dev)
 {
 	kfree(btrtl_dev->fw_data);
@@ -515,7 +601,7 @@ struct btrtl_device_info *btrtl_initialize(struct hci_dev *hdev,
 	struct hci_rp_read_local_version *resp;
 	char cfg_name[40];
 	u16 hci_rev, lmp_subver;
-	u8 hci_ver;
+	u8 hci_ver, chip_type = 0;
 	int ret;
 
 	btrtl_dev = kzalloc(sizeof(*btrtl_dev), GFP_KERNEL);
@@ -540,8 +626,14 @@ struct btrtl_device_info *btrtl_initialize(struct hci_dev *hdev,
 	lmp_subver = le16_to_cpu(resp->lmp_subver);
 	kfree_skb(skb);
 
+	if (rtl_has_chip_type(lmp_subver)) {
+		ret = rtl_read_chip_type(hdev, &chip_type);
+		if (ret)
+			goto err_free;
+	}
+
 	btrtl_dev->ic_info = btrtl_match_ic(lmp_subver, hci_rev, hci_ver,
-					    hdev->bus);
+					    hdev->bus, chip_type);
 
 	if (!btrtl_dev->ic_info) {
 		rtl_dev_err(hdev, "rtl: unknown IC info, lmp subver %04x, hci rev %04x, hci ver %04x",
@@ -610,6 +702,7 @@ int btrtl_download_firmware(struct hci_dev *hdev,
 	case RTL_ROM_LMP_8821A:
 	case RTL_ROM_LMP_8761A:
 	case RTL_ROM_LMP_8822B:
+	case RTL_ROM_LMP_8703B:
 		return btrtl_setup_rtl8723b(hdev, btrtl_dev);
 	default:
 		rtl_dev_info(hdev, "rtl: assuming no firmware upload needed\n");
@@ -628,7 +721,12 @@ int btrtl_setup_realtek(struct hci_dev *hdev)
 		return PTR_ERR(btrtl_dev);
 
 	ret = btrtl_download_firmware(hdev, btrtl_dev);
+	if (ret)
+		goto out_free;
 
+	btrtl_apply_quirks(hdev, btrtl_dev);
+
+out_free:
 	btrtl_free(btrtl_dev);
 
 	return ret;
@@ -743,6 +841,24 @@ int btrtl_get_uart_settings(struct hci_dev *hdev,
 }
 EXPORT_SYMBOL_GPL(btrtl_get_uart_settings);
 
+void btrtl_apply_quirks(struct hci_dev *hdev,
+			struct btrtl_device_info *btrtl_dev)
+{
+	switch (btrtl_dev->ic_info->lmp_subver) {
+	case RTL_ROM_LMP_8703B:
+		/* 8723CS reports two pages for local ext features,
+		 * but it doesn't support any features from page 2 -
+		 * it either responds with garbage or with error status
+		 */
+		set_bit(HCI_QUIRK_BROKEN_LOCAL_EXT_FTR_MAX_PAGE,
+			&hdev->quirks);
+		break;
+	default:
+		break;
+	}
+}
+EXPORT_SYMBOL_GPL(btrtl_apply_quirks);
+
 MODULE_AUTHOR("Daniel Drake <drake@endlessm.com>");
 MODULE_DESCRIPTION("Bluetooth support for Realtek devices ver " VERSION);
 MODULE_VERSION(VERSION);
@@ -752,6 +868,12 @@ MODULE_FIRMWARE("rtl_bt/rtl8723b_fw.bin");
 MODULE_FIRMWARE("rtl_bt/rtl8723b_config.bin");
 MODULE_FIRMWARE("rtl_bt/rtl8723bs_fw.bin");
 MODULE_FIRMWARE("rtl_bt/rtl8723bs_config.bin");
+MODULE_FIRMWARE("rtl_bt/rtl8723cs_cg_fw.bin");
+MODULE_FIRMWARE("rtl_bt/rtl8723cs_cg_config.bin");
+MODULE_FIRMWARE("rtl_bt/rtl8723cs_vf_fw.bin");
+MODULE_FIRMWARE("rtl_bt/rtl8723cs_vf_config.bin");
+MODULE_FIRMWARE("rtl_bt/rtl8723cs_xx_fw.bin");
+MODULE_FIRMWARE("rtl_bt/rtl8723cs_xx_config.bin");
 MODULE_FIRMWARE("rtl_bt/rtl8723ds_fw.bin");
 MODULE_FIRMWARE("rtl_bt/rtl8723ds_config.bin");
 MODULE_FIRMWARE("rtl_bt/rtl8761a_fw.bin");
diff --git a/drivers/bluetooth/btrtl.h b/drivers/bluetooth/btrtl.h
index f5e36f3993a8..db4e4a1542b7 100644
--- a/drivers/bluetooth/btrtl.h
+++ b/drivers/bluetooth/btrtl.h
@@ -24,6 +24,11 @@
 
 struct btrtl_device_info;
 
+struct rtl_chip_type_evt {
+	__u8 status;
+	__u8 type;
+} __packed;
+
 struct rtl_download_cmd {
 	__u8 index;
 	__u8 data[RTL_FRAG_LEN];
@@ -69,6 +74,8 @@ int btrtl_get_uart_settings(struct hci_dev *hdev,
 			    struct btrtl_device_info *btrtl_dev,
 			    unsigned int *controller_baudrate,
 			    u32 *device_baudrate, bool *flow_control);
+void btrtl_apply_quirks(struct hci_dev *hdev,
+			struct btrtl_device_info *btrtl_dev);
 
 #else
 
@@ -100,6 +107,11 @@ static inline int btrtl_get_uart_settings(struct hci_dev *hdev,
 					  bool *flow_control)
 {
 	return -ENOENT;
+
+static inline void btrtl_apply_quirks(struct hci_dev *hdev,
+			struct btrtl_device_info *btrtl_dev)
+{
+}
 }
 
 #endif
diff --git a/drivers/bluetooth/hci_h5.c b/drivers/bluetooth/hci_h5.c
index 9cc10e299fa8..7d72e092ce9d 100644
--- a/drivers/bluetooth/hci_h5.c
+++ b/drivers/bluetooth/hci_h5.c
@@ -892,6 +892,10 @@ static int h5_btrtl_setup(struct h5 *h5)
 	err = btrtl_download_firmware(h5->hu->hdev, btrtl_dev);
 	/* Give the device some time before the hci-core sends it a reset */
 	usleep_range(10000, 20000);
+	if (err)
+		goto out_free;
+
+	btrtl_apply_quirks(h5->hu->hdev, btrtl_dev);
 
 out_free:
 	btrtl_free(btrtl_dev);
-- 
2.17.1

