From ba9ba2949e86b5a00b0ae89b5e298b4cd46118ee Mon Sep 17 00:00:00 2001
From: wuweidong <625769020@qq.com>
Date: Mon, 27 Nov 2017 10:23:51 +0800
Subject: [PATCH] arm64: dts: sun50i-h5-nanopi: Add a new board NanoPi K1 Plus

---
 arch/arm64/boot/dts/allwinner/Makefile        |   1 +
 .../allwinner/sun50i-h5-nanopi-k1-plus.dts    | 555 ++++++++++++++++++
 2 files changed, 556 insertions(+)
 create mode 100644 arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-k1-plus.dts

diff --git a/arch/arm64/boot/dts/allwinner/Makefile b/arch/arm64/boot/dts/allwinner/Makefile
index c03224962034..eb4494332002 100644
--- a/arch/arm64/boot/dts/allwinner/Makefile
+++ b/arch/arm64/boot/dts/allwinner/Makefile
@@ -10,6 +10,7 @@ dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-pinebook.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-sopine-baseboard.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-teres-i.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-orangepi-pc2.dtb
+dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-nanopi-k1-plus.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-orangepi-prime.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-orangepi-zero-plus.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-orangepi-zero-plus2.dtb
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-k1-plus.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-k1-plus.dts
new file mode 100644
index 000000000000..52337a18721f
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-k1-plus.dts
@@ -0,0 +1,367 @@
+/*
+ * Copyright (C) 2016 ARM Ltd.
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This file is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+/dts-v1/;
+#include "sun50i-h5.dtsi"
+
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/input/input.h>
+#include <dt-bindings/pinctrl/sun4i-a10.h>
+
+/ {
+	model = "FriendlyElec NanoPi K1 Plus";
+	compatible = "friendlyelec,nanopi-k1-plus", "allwinner,sun50i-h5";
+
+	reg_vcc3v3: vcc3v3 {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+	};
+
+	aliases {
+		ethernet0 = &emac;
+		serial0 = &uart0;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	connector {
+		compatible = "hdmi-connector";
+		type = "a";
+
+		port {
+			hdmi_con_in: endpoint {
+				remote-endpoint = <&hdmi_out_con>;
+			};
+		};
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		status {
+			label = "nanopi:green:status";
+			gpios = <&pio 0 10 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "heartbeat";
+			};
+		pwr {
+			label = "nanopi:red:pwr";
+			gpios = <&r_pio 0 10 GPIO_ACTIVE_HIGH>;
+			default-state = "on";
+		};
+
+	};
+
+	r-gpio-keys {
+		compatible = "gpio-keys";
+
+		sw4 {
+			label = "sw4";
+			linux,code = <BTN_0>;
+			gpios = <&r_pio 0 3 GPIO_ACTIVE_LOW>;
+		};
+	};
+
+	reg_gmac_3v3: gmac-3v3 {
+		compatible = "regulator-fixed";
+		pinctrl-names = "default";
+		pinctrl-0 = <&gmac_power_pin_nanopi>;
+		regulator-name = "gmac-3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		startup-delay-us = <100000>;
+		enable-active-high;
+		gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>;
+	};
+
+	reg_usb0_vbus: usb0-vbus {
+		compatible = "regulator-fixed";
+		regulator-name = "usb0-vbus";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		enable-active-high;
+		gpio = <&r_pio 0 2 GPIO_ACTIVE_HIGH>; /* PL2 */
+		status = "okay";
+	};
+
+	wifi_pwrseq: wifi_pwrseq {
+        compatible = "mmc-pwrseq-simple";
+        pinctrl-names = "default";
+        pinctrl-0 = <&wifi_en_npi>;
+        reset-gpios = <&r_pio 0 7 GPIO_ACTIVE_LOW>; /* PL7 */
+        post-power-on-delay-ms = <200>;
+    };
+
+	rfkill_bt {
+		compatible = "rfkill-gpio";
+		pinctrl-names = "default";
+		pinctrl-0 = <&bt_pwr_pin>;
+		reset-gpios = <&pio 6 13 GPIO_ACTIVE_HIGH>; /* PG13 */
+		clocks = <&osc32k>;
+		clock-frequency = <32768>;
+		rfkill-name = "sunxi-bt";
+		rfkill-type = "bluetooth";
+	};
+
+	pcm5102a: pcm5102a-codec {
+        #sound-dai-cells = <0>;
+        compatible = "ti,pcm5102a";
+        status = "disabled";
+    };
+};
+
+&codec {
+	allwinner,audio-routing =
+		"Line Out", "LINEOUT",
+		"MIC1", "Mic",
+		"Mic",  "MBIAS";
+	status = "okay";
+};
+
+&de {
+	status = "okay";
+};
+
+&ehci0 {
+	status = "okay";
+};
+
+&ehci1 {
+	status = "okay";
+};
+
+&ehci2 {
+	status = "okay";
+};
+
+&ehci3 {
+	status = "okay";
+};
+
+&external_mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <0>;
+	};
+};
+
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_gmac_3v3>;
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii";
+	local-mac-address = [ 00 00 00 00 00 00 ];
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
+&ir {
+	pinctrl-names = "default";
+	pinctrl-0 = <&ir_pins_a>;
+	status = "okay";
+};
+
+&mmc0 {
+	vmmc-supply = <&reg_vcc3v3>;
+	bus-width = <4>;
+	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>; /* PF6 */
+	status = "okay";
+};
+
+&mmc1 {
+    vmmc-supply = <&reg_vcc3v3>;
+    vqmmc-supply = <&reg_vcc3v3>;
+    mmc-pwrseq = <&wifi_pwrseq>;
+    bus-width = <4>;
+    non-removable;
+    status = "okay";
+    brcmf: bcrmf@1 {
+        reg = <1>;
+        compatible = "brcm,bcm4329-fmac";
+    };
+};
+
+&mmc2 {
+    vmmc-supply = <&reg_vcc3v3>;
+    bus-width = <8>;
+    non-removable;
+    cap-mmc-hw-reset;
+    boot_device = <0>;
+    status = "okay";
+};
+
+&mmc2_8bit_pins {
+    /* Increase drive strength for DDR modes */
+    drive-strength = <40>;
+    /* eMMC is missing pull-ups */
+    bias-pull-up;
+};
+
+&hdmi {
+	status = "okay";
+};
+
+&hdmi_out {
+	hdmi_out_con: endpoint {
+		remote-endpoint = <&hdmi_con_in>;
+	};
+};
+
+
+&pio {
+	leds_npi: led_pins@0 {
+		pins = "PA10";
+		function = "gpio_out";
+	};
+	gmac_power_pin_nanopi: gmac_power_pin@0 {
+		pins = "PD6";
+		function = "gpio_out";
+	};
+	bt_pwr_pin: bt_pwr_pin@0 {
+		pins = "PG13";
+		function = "gpio_out";
+	};
+	spi0_cs_pins: spi0_cs_pins {
+        pins = "PC3", "PA6";
+        function = "gpio_out";
+    };
+};
+&r_pio {
+	leds_r_npi: led_pins@0 {
+		pins = "PL10";
+		function = "gpio_out";
+	};
+	vdd_cpux_r_npi: regulator_pins@0 {
+		allwinner,pins = "PL6";
+		allwinner,function = "gpio_out";
+		allwinner,drive = <SUN4I_PINCTRL_10_MA>;
+		allwinner,pull = <SUN4I_PINCTRL_NO_PULL>;
+	};
+	wifi_en_npi: wifi_en_pin {
+        pins = "PL7";
+        function = "gpio_out";
+    };
+};
+&ohci0 {
+	status = "okay";
+};
+
+&ohci1 {
+	status = "okay";
+};
+
+&ohci2 {
+	status = "okay";
+};
+
+&ohci3 {
+	status = "okay";
+};
+
+&spi0 {
+	status = "okay";
+        spi-flash@0 {
+                #address-cells = <1>;
+                #size-cells = <0>;
+                compatible = "jedec,spi-nor";
+                reg = <0>; /* Chip select 0 */
+                spi-max-frequency = <10000000>;
+                status = "okay";
+                partitions {
+                        compatible = "fixed-partitions";
+                        #address-cells = <1>;
+                        #size-cells = <1>;
+                        partition@0 {
+                                label = "uboot";
+                                reg = <0x0 0x100000>;
+                        };
+                        partition@100000 {
+                                label = "env";
+                                reg = <0x100000 0x100000>;
+                        };
+                };
+        };
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_pins_a>;
+	status = "okay";
+};
+
+&uart1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart1_pins>;
+	status = "disabled";
+};
+
+&uart2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart2_pins>;
+	status = "disabled";
+};
+
+&uart3 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart3_pins>, <&uart3_rts_cts_pins>;
+	status = "okay";
+};
+&usb_otg {
+	dr_mode = "otg";
+	status = "okay";
+};
+
+&usbphy {
+	/* USB Type-A ports' VBUS is always on */
+	usb0_id_det-gpios = <&pio 6 12 GPIO_ACTIVE_HIGH>; /* PG12 */
+	usb0_vbus-supply = <&reg_usb0_vbus>;
+	status = "okay";
+};
+
+&i2s0 {
+	sound-dai = <&pcm5102a>;
+	status = "disabled";
+};
\ No newline at end of file
