diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-nanopi-a64.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-nanopi-a64.dts
index 98dbff19f5cc..5caba225b4f7 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-nanopi-a64.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-nanopi-a64.dts
@@ -125,9 +125,9 @@
 
 &reg_dcdc1 {
 	regulator-always-on;
-	regulator-min-microvolt = <3000000>;
-	regulator-max-microvolt = <3000000>;
-	regulator-name = "vcc-3v";
+	regulator-min-microvolt = <3300000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "vcc-3v3";
 };
 
 &reg_dcdc2 {
