diff --git a/arch/arm/boot/dts/Makefile b/arch/arm/boot/dts/Makefile
index 093d09f9b..b5cd07dbd 100644
--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -1041,6 +1041,8 @@ dtb-$(CONFIG_MACH_SUN8I) += \
 	sun8i-h3-nanopi-m1-plus.dtb \
 	sun8i-h3-nanopi-neo.dtb \
 	sun8i-h3-nanopi-neo-air.dtb \
+	sun8i-h3-nanopi-r1.dtb \
+	sun8i-h3-nanopi-duo2.dtb \
 	sun8i-h3-orangepi-2.dtb \
 	sun8i-h3-orangepi-lite.dtb \
 	sun8i-h3-orangepi-one.dtb \
diff --git a/arch/arm/boot/dts/sun8i-h3-nanopi-r1.dts b/arch/arm/boot/dts/sun8i-h3-nanopi-r1.dts
new file mode 100644
index 000000000..731c705a4
--- /dev/null
+++ b/arch/arm/boot/dts/sun8i-h3-nanopi-r1.dts
@@ -0,0 +1,189 @@
+/*
+ * Copyright (C) 2019 Igor Pecovnik <igor@armbian.com>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This file is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+#include "sun8i-h3-nanopi.dtsi"
+
+/ {
+	model = "FriendlyElec NanoPi-R1";
+	compatible = "friendlyarm,nanopi-r1", "allwinner,sun8i-h3";
+
+	aliases {
+		serial1 = &uart3;
+		ethernet0 = &emac;
+		ethernet1 = &emac;
+		ethernet2 = &sdio_wifi;
+	};
+
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		pinctrl-names = "default";
+		reset-gpios = <&r_pio 0 7 GPIO_ACTIVE_LOW>; /* PL7 */
+	};
+
+	reg_gmac_3v3: gmac-3v3 {
+		compatible = "regulator-fixed";
+		regulator-name = "gmac-3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		startup-delay-us = <100000>;
+		enable-active-high;
+		gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>;
+	};
+
+	rfkill_bt {
+		compatible = "rfkill-gpio";
+		pinctrl-names = "default";
+		pinctrl-0 = <&bt_pwr_pin>;
+		reset-gpios = <&pio 6 13 GPIO_ACTIVE_HIGH>; /* PG13 */
+		clocks = <&osc32k>;
+		clock-frequency = <32768>;
+		rfkill-name = "sunxi-bt";
+		rfkill-type = "bluetooth";
+	};
+
+	leds {
+		/delete-node/ status;
+		/delete-node/ pwr;
+		led1 {
+			label = "LED1";
+			gpios = <&pio 0 10 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "heartbeat";
+		};
+
+		led2 {
+			label = "LED2";
+			gpios = <&pio 6 11 GPIO_ACTIVE_HIGH>;
+			default-state = "off";
+			linux,default-trigger = "netdev";
+		};
+
+		led3 {
+			label = "LED3";
+			gpios = <&pio 0 9 GPIO_ACTIVE_HIGH>;
+			default-state = "off";
+			linux,default-trigger = "netdev";
+		};
+	};
+
+	r_gpio_keys {
+		compatible = "gpio-keys";
+		input-name = "k1";
+		pinctrl-names = "default";
+		pinctrl-0 = <&sw_r_npi>;
+
+		/delete-node/ k1;
+		reset {
+			label = "reset";
+			linux,code = <BTN_1>;
+			gpios = <&r_pio 0 3 GPIO_ACTIVE_LOW>;
+		};
+	};
+};
+
+
+&pio {
+	bt_pwr_pin: bt_pwr_pin@0 {
+		pins = "PG13";
+		function = "gpio_out";
+	};
+};
+
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_gmac_3v3>;
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii";
+
+	status = "okay";
+};
+
+&external_mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <7>;
+	};
+};
+
+&mmc1 {
+	vmmc-supply = <&reg_vcc3v3>;
+	vqmmc-supply = <&reg_vcc3v3>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+
+	sdio_wifi: sdio_wifi@1 {
+		reg = <1>;
+		compatible = "brcm,bcm4329-fmac";
+		interrupt-parent = <&pio>;
+		interrupts = <6 10 IRQ_TYPE_LEVEL_LOW>; /* PG10 / EINT10 */
+		interrupt-names = "host-wake";
+	};
+};
+
+&mmc2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc2_8bit_pins>;
+	vmmc-supply = <&reg_vcc3v3>;
+	vqmmc-supply = <&reg_vcc3v3>;
+	bus-width = <8>;
+	non-removable;
+	status = "okay";
+};
+
+&ohci0 {
+	status = "okay";
+};
+
+&ohci1 {
+	status = "okay";
+};
+
+&usb_otg {
+	dr_mode = "peripheral";
+	status = "okay";
+};
+
+&usbphy {
+	status = "okay";
+};
diff --git a/arch/arm/boot/dts/sun8i-h3-nanopi-duo2.dts b/arch/arm/boot/dts/sun8i-h3-nanopi-duo2.dts
new file mode 100644
index 000000000..34d173afe
--- /dev/null
+++ b/arch/arm/boot/dts/sun8i-h3-nanopi-duo2.dts
@@ -0,0 +1,97 @@
+/*
+ * Copyright (C) 2019 Igor <igor@armbian.com>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This file is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+#include "sun8i-h3-nanopi.dtsi"
+
+/ {
+	model = "FriendlyElec NanoPi-Duo2";
+	compatible = "friendlyarm,nanopi-duo2", "allwinner,sun8i-h3";
+
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		pinctrl-names = "default";
+		reset-gpios = <&r_pio 0 7 GPIO_ACTIVE_LOW>; /* PL7 */
+		post-power-on-delay-ms = <200>;
+	};
+
+};
+
+&r_pio {
+	wifi_en_npi: wifi_en_pin {
+		pins = "PL7";
+		function = "gpio_out";
+	};
+};
+
+&mmc1 {
+	vmmc-supply = <&reg_vcc3v3>;
+	vqmmc-supply = <&reg_vcc3v3>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+
+	sdio_wifi: sdio_wifi@1 {
+		reg = <1>;
+		compatible = "brcm,bcm4329-fmac";
+		interrupt-parent = <&pio>;
+		interrupts = <6 10 IRQ_TYPE_LEVEL_LOW>; /* PG10 / EINT10 */
+		interrupt-names = "host-wake";
+	};
+
+};
+
+&emac {
+	phy-handle = <&int_mii_phy>;
+	phy-mode = "mii";
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
+&usb_otg {
+	dr_mode = "peripheral";
+	status = "okay";
+};
+
+&usbphy {
+	status = "okay";
+};
