diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus2.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus2.dts
index 50ad2e4fd..e1ee1cd09 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus2.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus2.dts
@@ -98,6 +98,27 @@
 			linux,default-trigger = "heartbeat";
 		};
 	};
+
+	reg_vdd_cpux: gpio-regulator {
+		compatible = "regulator-gpio";
+		regulator-name = "vdd-cpux";
+		regulator-type = "voltage";
+		regulator-boot-on;
+		regulator-always-on;
+		regulator-min-microvolt = <1108475>;
+		regulator-max-microvolt = <1307810>;
+		regulator-ramp-delay = <50>; /* 4ms */
+		enable-gpios =  <&r_pio 0 8 GPIO_ACTIVE_HIGH>; /* PL8 */
+		gpios = <&r_pio 0 6 0>; /* PL6 */
+		enable-active-high;
+		gpios-states = <0x1>;
+		states = <1108475 0x0
+			  1307810 0x1>;
+	};
+};
+
+&cpu0 {
+	cpu-supply = <&reg_vdd_cpux>;
 };
 
 &de {
