diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi
index 67e2246a6..e37d779f8 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi
@@ -55,7 +55,6 @@
 			clocks = <&ccu CLK_CPUX>;
 			clock-names = "cpu";
 			operating-points-v2 = <&cpu0_opp_table>;
-			clock-frequency = <1200000000>;
 			#cooling-cells = <2>;
 			cooling-min-level = <0>;
 			cooling-max-level = <15>;
@@ -67,7 +66,6 @@
 			reg = <1>;
 			enable-method = "psci";
 			operating-points-v2 = <&cpu0_opp_table>;
-			clock-frequency = <1200000000>;
 		};
 
 		cpu@2 {
@@ -76,7 +74,6 @@
 			reg = <2>;
 			enable-method = "psci";
 			operating-points-v2 = <&cpu0_opp_table>;
-			clock-frequency = <1200000000>;
 		};
 
 		cpu@3 {
@@ -85,10 +82,16 @@
 			reg = <3>;
 			enable-method = "psci";
 			operating-points-v2 = <&cpu0_opp_table>;
-			clock-frequency = <1200000000>;
 		};
 	};
 
+	reg_cpu_fallback: reg_cpu_fallback  {
+		compatible = "regulator-fixed";
+		regulator-name = "vdd-cpux-dummy";
+		regulator-min-microvolt = <1100000>;
+		regulator-max-microvolt = <1100000>;
+	};
+
 	psci {
 		compatible = "arm,psci-0.2";
 		method = "smc";
