diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-nanopi-a64.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-nanopi-a64.dts
index 1eba1324e5b9..5e3dc2666d0f 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-nanopi-a64.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-nanopi-a64.dts
@@ -58,6 +58,11 @@
 	chosen {
 		stdout-path = "serial0:115200n8";
 	};
+
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		reset-gpios = <&r_pio 0 2 GPIO_ACTIVE_LOW>; /* PL2 */
+	};
 };
 
 &ehci0 {
@@ -105,6 +110,24 @@
 	status = "okay";
 };
 
+&mmc1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc1_pins>;
+	vmmc-supply = <&reg_dcdc1>;
+	vqmmc-supply = <&reg_dldo4>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+
+	rtl8189etv: wifi@1 {
+		reg = <1>;
+		interrupt-parent = <&r_pio>;
+		interrupts = <0 3 IRQ_TYPE_LEVEL_LOW>; /* PL3 */
+		interrupt-names = "host-wake";
+	};
+};
+
 &ohci0 {
 	status = "okay";
 };
