From 7e268d45be35f4355b8088980820da1858058d2b Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Sun, 12 Nov 2017 19:03:08 +0100
Subject: [PATCH 53/82] ARM: dts: suni-a83t: Add support for I2S controller

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm/boot/dts/sun8i-a83t.dtsi | 13 +++++++++++++
 1 file changed, 13 insertions(+)

diff --git a/arch/arm/boot/dts/sun8i-a83t.dtsi b/arch/arm/boot/dts/sun8i-a83t.dtsi
index a8ff7a8efe71..147f76a66a28 100644
--- a/arch/arm/boot/dts/sun8i-a83t.dtsi
+++ b/arch/arm/boot/dts/sun8i-a83t.dtsi
@@ -304,6 +304,19 @@
 		#size-cells = <1>;
 		ranges;
 
+		dai: dai@01c23000 {
+			#sound-dai-cells = <0>;
+			compatible = "allwinner,sun8i-a83t-i2s";
+			reg = <0x01c23000 0x200>;
+			interrupts = <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_TDM>, <&ccu CLK_TDM>;
+			clock-names = "apb", "mod";
+			resets = <&ccu RST_BUS_TDM>;
+			dmas = <&dma 28>, <&dma 28>;
+			dma-names = "rx", "tx";
+			status = "disabled";
+		};
+
 		display_clocks: clock@1000000 {
 			compatible = "allwinner,sun8i-a83t-de2-clk";
 			reg = <0x01000000 0x100000>;
-- 
2.20.1

