From 87020e638ad511e0ebe9c72208d2f0192c905812 Mon Sep 17 00:00:00 2001
From: Vasily Khoruzhick <anarsoul@gmail.com>
Date: Sun, 3 Dec 2017 11:43:08 -0800
Subject: [PATCH 007/146] Add sopine HDMI sound and WiFi support

---
 .../allwinner/sun50i-a64-sopine-baseboard.dts | 18 ++++++++++++
 arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi | 29 +++++++++++++++++++
 2 files changed, 47 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-sopine-baseboard.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-sopine-baseboard.dts
index c21f2331add6..8161895dde52 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-sopine-baseboard.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-sopine-baseboard.dts
@@ -86,6 +86,10 @@
 	status = "okay";
 };
 
+&i2s2 {
+	status = "okay";
+};
+
 &mdio {
 	ext_rgmii_phy: ethernet-phy@1 {
 		compatible = "ethernet-phy-ieee802.3-c22";
@@ -93,6 +97,16 @@
 	};
 };
 
+&mmc1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc1_pins>;
+	vmmc-supply = <&reg_dldo4>;
+	vqmmc-supply = <&reg_eldo1>;
+	non-removable;
+	bus-width = <4>;
+	status = "okay";
+};
+
 &mmc2 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc2_pins>;
@@ -138,6 +152,10 @@
 	vcc-hdmi-supply = <&reg_dldo1>;
 };
 
+&sound_hdmi {
+	status = "okay";
+};
+
 &uart0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart0_pins_a>;
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
index 0f69f3593975..0b44018361cb 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
@@ -727,6 +727,35 @@
 			status = "disabled";
 		};
 
+		i2s2: i2s@1c22800 {
+			#sound-dai-cells = <0>;
+			compatible = "allwinner,sun8i-h3-i2s";
+			reg = <0x01c22800 0x400>;
+			interrupts = <GIC_SPI 15 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2S2>, <&ccu CLK_I2S2>;
+			clock-names = "apb", "mod";
+			dmas = <&dma 27>;
+			resets = <&ccu RST_BUS_I2S2>;
+			dma-names = "tx";
+			status = "disabled";
+		};
+
+		sound_hdmi: sound_hdmi {
+			compatible = "simple-audio-card";
+			simple-audio-card,format = "i2s";
+			simple-audio-card,name = "allwinner,hdmi";
+			simple-audio-card,mclk-fs = <256>;
+			status = "disabled";
+
+			simple-audio-card,codec {
+				sound-dai = <&hdmi>;
+			};
+
+			simple-audio-card,cpu {
+				sound-dai = <&i2s2>;
+			};
+		};
+
 		rtc: rtc@1f00000 {
 			compatible = "allwinner,sun6i-a31-rtc";
 			reg = <0x01f00000 0x54>;
-- 
2.17.1

