diff --git a/arch/arm/boot/dts/sunxi-h3-h5.dtsi b/arch/arm/boot/dts/sunxi-h3-h5.dtsi
index 586ce53fc..e72c24470 100644
--- a/arch/arm/boot/dts/sunxi-h3-h5.dtsi
+++ b/arch/arm/boot/dts/sunxi-h3-h5.dtsi
@@ -590,19 +590,6 @@
 			};
 		};
 
-		ths: ths@1c25000 {
-			#thermal-sensor-cells = <0>;
-			compatible = "allwinner,sun8i-h3-ths";
-			reg = <0x01c25000 0x400>,
-			      <0x01c14234 0x4>;
-			reg-names = "ths", "calibration";
-			interrupts = <GIC_SPI 31 IRQ_TYPE_LEVEL_HIGH>;
-			resets = <&ccu RST_BUS_THS>;
-			reset-names = "ahb";
-			clocks = <&ccu CLK_BUS_THS>, <&ccu CLK_THS>;
-			clock-names = "ahb", "ths";
-		};
-
 		timer@1c20c00 {
 			compatible = "allwinner,sun4i-a10-timer";
 			reg = <0x01c20c00 0xa0>;
