From d0970394839f5b09d564142c8a4687ef64458586 Mon Sep 17 00:00:00 2001
From: Vasily Khoruzhick <anarsoul@gmail.com>
Date: Sun, 3 Dec 2017 11:40:25 -0800
Subject: [PATCH 122/146] arm64: dts: allwinner: a64: enable sound on Pinebook

This commit enables I2S, digital and analog parts of audiocodec on
Pinebook

Signed-off-by: Vasily Khoruzhick <anarsoul@gmail.com>
---
 .../dts/allwinner/sun50i-a64-pinebook.dts     | 42 +++++++++++++++++++
 1 file changed, 42 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinebook.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinebook.dts
index dce16d9d6afb..b55ac4e1df37 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pinebook.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pinebook.dts
@@ -71,16 +71,33 @@
 		regulator-max-microvolt = <3300000>;
 	};
 
+	speaker_amp: speaker_amp {
+		compatible = "simple-audio-amplifier";
+		enable-gpios = <&pio 7 7 GPIO_ACTIVE_HIGH>;
+	};
+
 	wifi_pwrseq: wifi_pwrseq {
 		compatible = "mmc-pwrseq-simple";
 		reset-gpios = <&r_pio 0 2 GPIO_ACTIVE_LOW>; /* PL2 */
 	};
 };
 
+&codec {
+	status = "okay";
+};
+
+&codec_analog {
+	status = "okay";
+};
+
 &cpu0 {
        cpu-supply = <&reg_dcdc2>;
 };
 
+&dai {
+	status = "okay";
+};
+
 &de {
 	status = "okay";
 };
@@ -306,6 +323,31 @@
 	vcc-hdmi-supply = <&reg_dldo1>;
 };
 
+&sound {
+	status = "okay";
+	simple-audio-card,widgets = "Microphone", "Internal Microphone Left",
+				    "Microphone", "Internal Microphone Right",
+				    "Headphone", "Headphone Jack",
+				    "Speaker", "Internal Speaker";
+	simple-audio-card,aux-devs = <&codec_analog>, <&speaker_amp>;
+	simple-audio-card,routing =
+			"Left DAC", "AIF1 Slot 0 Left",
+			"Right DAC", "AIF1 Slot 0 Right",
+			"INL", "LINEOUT",
+			"INR", "LINEOUT",
+			"Internal Speaker", "OUTL",
+			"Internal Speaker", "OUTR",
+			"Headphone Jack", "HP",
+			"AIF1 Slot 0 Left ADC", "Left ADC",
+			"AIF1 Slot 0 Right ADC", "Right ADC",
+			"Left ADC", "ADC",
+			"Right ADC", "ADC",
+			"Internal Microphone Left", "MBIAS",
+			"MIC1", "Internal Microphone Left",
+			"Internal Microphone Right", "HBIAS",
+			"MIC2", "Internal Microphone Right";
+};
+
 &uart0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart0_pins_a>;
-- 
2.17.1

