From 379fee744cb1fa4370ac692bc890e5e1182e337d Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Fri, 8 Dec 2017 12:44:22 +0100
Subject: [PATCH 62/82] ARM: dts: sun8i-a83t-tbs: Increase voltage on the
 vibrator

To make it less sluggish.

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts | 4 ++--
 1 file changed, 2 insertions(+), 2 deletions(-)

diff --git a/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts b/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
index 99c5df15b036..ea7b8bf4d327 100644
--- a/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
+++ b/arch/arm/boot/dts/sun8i-a83t-tbs-a711.dts
@@ -608,8 +608,8 @@
 };
 
 &reg_ldo_io1 {
-	regulator-min-microvolt = <3100000>;
-	regulator-max-microvolt = <3100000>;
+	regulator-min-microvolt = <3300000>;
+	regulator-max-microvolt = <3300000>;
 	regulator-name = "vcc-vb";
 	status = "okay";
 };
-- 
2.20.1

