diff --git a/arch/arm64/boot/dts/allwinner/Makefile b/arch/arm64/boot/dts/allwinner/Makefile
index c6fc096..731e2ae 100644
--- a/arch/arm64/boot/dts/allwinner/Makefile
+++ b/arch/arm64/boot/dts/allwinner/Makefile
@@ -11,6 +11,7 @@ dtb-$(CONFIG_ARCH_SUNXI) += sun50i-a64-teres-i.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-libretech-all-h3-cc.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-nanopi-neo2.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-nanopi-neo-plus2.dtb
+dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-nanopi-neo-core2.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-orangepi-pc2.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-nanopi-k1-plus.dtb
 dtb-$(CONFIG_ARCH_SUNXI) += sun50i-h5-orangepi-prime.dtb
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo-core2.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo-core2.dts
new file mode 100644
index 000000000..b3035ddd7
--- /dev/null
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo-core2.dts
@@ -0,0 +1,210 @@
+/*
+ * Copyright (C) 2017 Antony Antony <antony@phenome.org>
+ * Copyright (C) 2016 ARM Ltd.
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This file is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+/dts-v1/;
+#include "sun50i-h5.dtsi"
+
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/input/input.h>
+#include <dt-bindings/pinctrl/sun4i-a10.h>
+
+/ {
+	model = "FriendlyARM NanoPi NEO Core2";
+	compatible = "friendlyarm,nanopi-neo-core2", "allwinner,sun50i-h5";
+
+	aliases {
+		ethernet0 = &emac;
+		serial0 = &uart0;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		pwr {
+			label = "nanopi:red:pwr";
+			gpios = <&r_pio 0 10 GPIO_ACTIVE_HIGH>; /* PL10 */
+			linux,default-trigger = "default-on";
+		};
+
+		status {
+			label = "nanopi:green:status";
+			gpios = <&pio 0 10 GPIO_ACTIVE_HIGH>; /* PA10 */
+			linux,default-trigger = "heartbeat";
+		};
+	};
+
+	reg_gmac_3v3: gmac-3v3 {
+		compatible = "regulator-fixed";
+		pinctrl-names = "default";
+		regulator-name = "gmac-3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+		startup-delay-us = <100000>;
+		enable-active-high;
+		gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>;
+	};
+
+	reg_vcc3v3: vcc3v3 {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+	};
+
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		pinctrl-names = "default";
+		reset-gpios = <&r_pio 0 7 GPIO_ACTIVE_LOW>; /* PL7 */
+		post-power-on-delay-ms = <200>;
+	};
+};
+
+&cpu0 {
+	cpu-supply = <&vdd_cpux>;
+};
+
+&codec {
+	allwinner,audio-routing =
+		"Line Out", "LINEOUT",
+		"MIC1", "Mic",
+		"Mic",  "MBIAS";
+	status = "okay";
+};
+
+&ehci0 {
+	status = "okay";
+};
+
+&ehci3 {
+	status = "okay";
+};
+
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_gmac_3v3>;
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii";
+	status = "okay";
+};
+
+&external_mdio {
+	ext_rgmii_phy: ethernet-phy@7 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <7>;
+	};
+};
+
+&mmc0 {
+	vmmc-supply = <&reg_vcc3v3>;
+	bus-width = <4>;
+	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>; /* PF6 */
+	status = "okay";
+};
+
+&mmc1 {
+	vmmc-supply = <&reg_vcc3v3>;
+	vqmmc-supply = <&reg_vcc3v3>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+
+	brcmf: wifi@1 {
+		reg = <1>;
+		compatible = "brcm,bcm4329-fmac";
+	};
+};
+
+&mmc2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc2_8bit_pins>;
+	vmmc-supply = <&reg_vcc3v3>;
+	bus-width = <8>;
+	non-removable;
+	cap-mmc-hw-reset;
+	status = "okay";
+};
+
+&ohci0 {
+	status = "okay";
+};
+
+&ohci3 {
+	status = "okay";
+};
+
+&r_i2c {
+	status = "okay";
+
+	vdd_cpux: regulator@65 {
+		compatible = "silergy,sy8106a";
+		reg = <0x65>;
+		silergy,fixed-microvolt = <1000000>;
+		regulator-min-microvolt = <1000000>;
+		regulator-max-microvolt = <1400000>;
+		regulator-ramp-delay = <200>;
+		regulator-boot-on;
+		regulator-always-on;
+	};
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_pins_a>;
+	status = "okay";
+};
+
+&usb_otg {
+	dr_mode = "host";
+	status = "okay";
+};
+
+&usbphy {
+	/* USB Type-A ports' VBUS is always on */
+	status = "okay";
+};
