From 9b5c2c835ee29d5dce19b1cffe42cc2b47b6ac01 Mon Sep 17 00:00:00 2001
From: Icenowy Zheng <icenowy@aosc.io>
Date: Sun, 3 Sep 2017 23:53:15 +0800
Subject: [PATCH] Revert "arm: dts: sunxi: Revert EMAC changes"

This reverts commit fe45174b72aead678da581bab9e9a37c9b26a070.

Signed-off-by: Icenowy Zheng <icenowy@aosc.io>
---
 arch/arm/boot/dts/sun8i-h2-plus-orangepi-zero.dts |  9 ++++++++
 arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts   | 19 +++++++++++++++++
 arch/arm/boot/dts/sun8i-h3-nanopi-neo.dts         |  7 ++++++
 arch/arm/boot/dts/sun8i-h3-orangepi-2.dts         |  8 +++++++
 arch/arm/boot/dts/sun8i-h3-orangepi-one.dts       |  8 +++++++
 arch/arm/boot/dts/sun8i-h3-orangepi-pc-plus.dts   |  5 +++++
 arch/arm/boot/dts/sun8i-h3-orangepi-pc.dts        |  8 +++++++
 arch/arm/boot/dts/sun8i-h3-orangepi-plus.dts      | 22 +++++++++++++++++++
 arch/arm/boot/dts/sun8i-h3-orangepi-plus2e.dts    | 16 ++++++++++++++
 arch/arm/boot/dts/sunxi-h3-h5.dtsi                | 26 +++++++++++++++++++++++
 10 files changed, 128 insertions(+)

diff --git a/arch/arm/boot/dts/sun8i-h2-plus-orangepi-zero.dts b/arch/arm/boot/dts/sun8i-h2-plus-orangepi-zero.dts
index b1502df7b5092..6713d0f2b3f4d 100644
--- a/arch/arm/boot/dts/sun8i-h2-plus-orangepi-zero.dts
+++ b/arch/arm/boot/dts/sun8i-h2-plus-orangepi-zero.dts
@@ -56,6 +56,8 @@
 
 	aliases {
 		serial0 = &uart0;
+		/* ethernet0 is the H3 emac, defined in sun8i-h3.dtsi */
+		ethernet0 = &emac;
 		ethernet1 = &xr819;
 	};
 
@@ -102,6 +104,13 @@
 	status = "okay";
 };
 
+&emac {
+	phy-handle = <&int_mii_phy>;
+	phy-mode = "mii";
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
 &mmc0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc0_pins_a>;
diff --git a/arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts b/arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts
index a337af1de3224..d756ff8251160 100644
--- a/arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts
+++ b/arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts
@@ -52,6 +52,7 @@
 	compatible = "sinovoip,bpi-m2-plus", "allwinner,sun8i-h3";
 
 	aliases {
+		ethernet0 = &emac;
 		serial0 = &uart0;
 		serial1 = &uart1;
 	};
@@ -114,12 +115,30 @@
 	status = "okay";
 };
 
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_gmac_3v3>;
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii";
+
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
 &ir {
 	pinctrl-names = "default";
 	pinctrl-0 = <&ir_pins_a>;
 	status = "okay";
 };
 
+&mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <0>;
+	};
+};
+
 &mmc0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc0_pins_a>, <&mmc0_cd_pin>;
diff --git a/arch/arm/boot/dts/sun8i-h3-nanopi-neo.dts b/arch/arm/boot/dts/sun8i-h3-nanopi-neo.dts
index 8d2cc6e9a03fa..78f6c24952dd1 100644
--- a/arch/arm/boot/dts/sun8i-h3-nanopi-neo.dts
+++ b/arch/arm/boot/dts/sun8i-h3-nanopi-neo.dts
@@ -46,3 +46,10 @@
 	model = "FriendlyARM NanoPi NEO";
 	compatible = "friendlyarm,nanopi-neo", "allwinner,sun8i-h3";
 };
+
+&emac {
+	phy-handle = <&int_mii_phy>;
+	phy-mode = "mii";
+	allwinner,leds-active-low;
+	status = "okay";
+};
diff --git a/arch/arm/boot/dts/sun8i-h3-orangepi-2.dts b/arch/arm/boot/dts/sun8i-h3-orangepi-2.dts
index 8ff71b1bb45b1..17cdeae19c6f0 100644
--- a/arch/arm/boot/dts/sun8i-h3-orangepi-2.dts
+++ b/arch/arm/boot/dts/sun8i-h3-orangepi-2.dts
@@ -54,6 +54,7 @@
 	aliases {
 		serial0 = &uart0;
 		/* ethernet0 is the H3 emac, defined in sun8i-h3.dtsi */
+		ethernet0 = &emac;
 		ethernet1 = &rtl8189;
 	};
 
@@ -117,6 +118,13 @@
 	status = "okay";
 };
 
+&emac {
+	phy-handle = <&int_mii_phy>;
+	phy-mode = "mii";
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
 &ir {
 	pinctrl-names = "default";
 	pinctrl-0 = <&ir_pins_a>;
diff --git a/arch/arm/boot/dts/sun8i-h3-orangepi-one.dts b/arch/arm/boot/dts/sun8i-h3-orangepi-one.dts
index 5fea430e0eb10..6880268e8b87b 100644
--- a/arch/arm/boot/dts/sun8i-h3-orangepi-one.dts
+++ b/arch/arm/boot/dts/sun8i-h3-orangepi-one.dts
@@ -52,6 +52,7 @@
 	compatible = "xunlong,orangepi-one", "allwinner,sun8i-h3";
 
 	aliases {
+		ethernet0 = &emac;
 		serial0 = &uart0;
 	};
 
@@ -97,6 +98,13 @@
 	status = "okay";
 };
 
+&emac {
+	phy-handle = <&int_mii_phy>;
+	phy-mode = "mii";
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
 &mmc0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc0_pins_a>, <&mmc0_cd_pin>;
diff --git a/arch/arm/boot/dts/sun8i-h3-orangepi-pc-plus.dts b/arch/arm/boot/dts/sun8i-h3-orangepi-pc-plus.dts
index 8b93f5c781a70..a10281b455f50 100644
--- a/arch/arm/boot/dts/sun8i-h3-orangepi-pc-plus.dts
+++ b/arch/arm/boot/dts/sun8i-h3-orangepi-pc-plus.dts
@@ -53,6 +53,11 @@
 	};
 };
 
+&emac {
+	/* LEDs changed to active high on the plus */
+	/delete-property/ allwinner,leds-active-low;
+};
+
 &mmc1 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc1_pins_a>;
diff --git a/arch/arm/boot/dts/sun8i-h3-orangepi-pc.dts b/arch/arm/boot/dts/sun8i-h3-orangepi-pc.dts
index 1a044b17d6c61..998b60f8d295e 100644
--- a/arch/arm/boot/dts/sun8i-h3-orangepi-pc.dts
+++ b/arch/arm/boot/dts/sun8i-h3-orangepi-pc.dts
@@ -52,6 +52,7 @@
 	compatible = "xunlong,orangepi-pc", "allwinner,sun8i-h3";
 
 	aliases {
+		ethernet0 = &emac;
 		serial0 = &uart0;
 	};
 
@@ -113,6 +114,13 @@
 	status = "okay";
 };
 
+&emac {
+	phy-handle = <&int_mii_phy>;
+	phy-mode = "mii";
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
 &ir {
 	pinctrl-names = "default";
 	pinctrl-0 = <&ir_pins_a>;
diff --git a/arch/arm/boot/dts/sun8i-h3-orangepi-plus.dts b/arch/arm/boot/dts/sun8i-h3-orangepi-plus.dts
index 828ae7a526d92..331ed683ac62c 100644
--- a/arch/arm/boot/dts/sun8i-h3-orangepi-plus.dts
+++ b/arch/arm/boot/dts/sun8i-h3-orangepi-plus.dts
@@ -47,6 +47,10 @@
 	model = "Xunlong Orange Pi Plus / Plus 2";
 	compatible = "xunlong,orangepi-plus", "allwinner,sun8i-h3";
 
+	aliases {
+		ethernet0 = &emac;
+	};
+
 	reg_gmac_3v3: gmac-3v3 {
 		compatible = "regulator-fixed";
 		regulator-name = "gmac-3v3";
@@ -74,6 +78,24 @@
 	status = "okay";
 };
 
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_gmac_3v3>;
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii";
+
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
+&mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <0>;
+	};
+};
+
 &mmc2 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc2_8bit_pins>;
diff --git a/arch/arm/boot/dts/sun8i-h3-orangepi-plus2e.dts b/arch/arm/boot/dts/sun8i-h3-orangepi-plus2e.dts
index 97920b12a9445..80026f3caafc8 100644
--- a/arch/arm/boot/dts/sun8i-h3-orangepi-plus2e.dts
+++ b/arch/arm/boot/dts/sun8i-h3-orangepi-plus2e.dts
@@ -61,3 +61,19 @@
 		gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>; /* PD6 */
 	};
 };
+
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_gmac_3v3>;
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii";
+	status = "okay";
+};
+
+&mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
+};
diff --git a/arch/arm/boot/dts/sunxi-h3-h5.dtsi b/arch/arm/boot/dts/sunxi-h3-h5.dtsi
index 11240a8313c26..d38282b9e5d44 100644
--- a/arch/arm/boot/dts/sunxi-h3-h5.dtsi
+++ b/arch/arm/boot/dts/sunxi-h3-h5.dtsi
@@ -391,6 +391,32 @@
 			clocks = <&osc24M>;
 		};
 
+		emac: ethernet@1c30000 {
+			compatible = "allwinner,sun8i-h3-emac";
+			syscon = <&syscon>;
+			reg = <0x01c30000 0x10000>;
+			interrupts = <GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "macirq";
+			resets = <&ccu RST_BUS_EMAC>;
+			reset-names = "stmmaceth";
+			clocks = <&ccu CLK_BUS_EMAC>;
+			clock-names = "stmmaceth";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+
+			mdio: mdio {
+				#address-cells = <1>;
+				#size-cells = <0>;
+				int_mii_phy: ethernet-phy@1 {
+					compatible = "ethernet-phy-ieee802.3-c22";
+					reg = <1>;
+					clocks = <&ccu CLK_BUS_EPHY>;
+					resets = <&ccu RST_BUS_EPHY>;
+				};
+			};
+		};
+
 		spi0: spi@01c68000 {
 			compatible = "allwinner,sun8i-h3-spi";
 			reg = <0x01c68000 0x1000>;
