diff --git a/arch/arm/boot/dts/sun8i-h3-nanopi-neo-air.dts b/arch/arm/boot/dts/sun8i-h3-nanopi-neo-air.dts
old mode 100644
new mode 100755
index 03ff6f8..ddbb92b
--- a/arch/arm/boot/dts/sun8i-h3-nanopi-neo-air.dts
+++ b/arch/arm/boot/dts/sun8i-h3-nanopi-neo-air.dts
@@ -47,7 +47,7 @@
 #include <dt-bindings/gpio/gpio.h>
 
 / {
-	model = "FriendlyARM NanoPi NEO Air";
+	model = "FriendlyElec NanoPi NEO Air";
 	compatible = "friendlyarm,nanopi-neo-air", "allwinner,sun8i-h3";
 
 	aliases {
@@ -58,6 +58,13 @@
 		stdout-path = "serial0:115200n8";
 	};
 
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		pinctrl-names = "default";
+		pinctrl-0 = <&wifi_en_neoair>;
+		reset-gpios = <&r_pio 0 7 GPIO_ACTIVE_LOW>; /* PL7 */
+	};
+
 	leds {
 		compatible = "gpio-leds";
 
@@ -70,10 +77,18 @@
 		status {
 			label = "nanopi:blue:status";
 			gpios = <&pio 0 10 GPIO_ACTIVE_HIGH>; /* PA10 */
+			linux,default-trigger = "heartbeat";
 		};
 	};
 };
 
+&r_pio {
+	wifi_en_neoair: wifi_en_pin@0 {
+		allwinner,pins = "PL7";
+		allwinner,function = "gpio_out";
+	};
+};
+
 &mmc0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc0_pins_a>, <&mmc0_cd_pin>;
@@ -84,6 +99,42 @@
 	status = "okay";
 };
 
+&mmc1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc1_pins_a>;
+	vmmc-supply = <&reg_vcc3v3>;
+	vqmmc-supply = <&reg_vcc3v3>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+
+	brcmf: bcrmf@1 {
+		reg = <1>;
+		compatible = "brcm,bcm4329-fmac";
+		interrupt-parent = <&pio>;
+		interrupts = <6 10 IRQ_TYPE_LEVEL_LOW>; /* PG10 / EINT10 */
+		interrupt-names = "host-wake";
+	};
+};
+
+&mmc2 {
+    pinctrl-names = "default";
+    pinctrl-0 = <&mmc2_8bit_pins>;
+    vmmc-supply = <&reg_vcc3v3>;
+    bus-width = <8>;
+    non-removable;
+    cap-mmc-hw-reset;
+    status = "okay";
+};
+
+&mmc2_8bit_pins {
+    /* Increase drive strength for DDR modes */
+    drive-strength = <40>;
+    /* eMMC is missing pull-ups */
+    bias-pull-up;
+};
+
 &uart0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart0_pins_a>;
