diff --git a/arch/arm/boot/dts/sunxi-h3-h5.dtsi b/arch/arm/boot/dts/sunxi-h3-h5.dtsi
index 5b82d160..bccfb98f 100644
--- a/arch/arm/boot/dts/sunxi-h3-h5.dtsi
+++ b/arch/arm/boot/dts/sunxi-h3-h5.dtsi
@@ -560,7 +560,7 @@
 
 		i2c2: i2c@01c2b400 {
 			compatible = "allwinner,sun6i-a31-i2c";
-			reg = <0x01c2b000 0x400>;
+			reg = <0x01c2b400 0x400>;
 			interrupts = <GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>;
 			clocks = <&ccu CLK_BUS_I2C2>;
 			resets = <&ccu RST_BUS_I2C2>;
