diff --git a/cmd/Kconfig b/cmd/Kconfig
index d6d130edfa..92795119ea 100644
--- a/cmd/Kconfig
+++ b/cmd/Kconfig
@@ -1029,6 +1029,7 @@ menu "Misc commands"
 config CMD_BMP
 	bool "Enable 'bmp' command"
 	depends on LCD || DM_VIDEO || VIDEO
+	default y
 	help
 	  This provides a way to obtain information about a BMP-format iamge
 	  and to display it. BMP (which presumably stands for BitMaP) is a
diff --git a/include/config_distro_bootcmd.h b/include/config_distro_bootcmd.h
index 9ed6b9892c..75d5176edf 100644
--- a/include/config_distro_bootcmd.h
+++ b/include/config_distro_bootcmd.h
@@ -323,6 +323,15 @@
 	BOOTENV_SHARED_UBIFS \
 	BOOTENV_SHARED_EFI \
 	"boot_prefixes=/ /boot/\0" \
+	"splashpos=m,m\0" \
+	"splashimage=66000000\0" \
+	"loadsplash= " \
+		"for prefix in ${boot_prefixes}; do " \
+			"if test -e mmc 0 ${prefix}boot.bmp; then " \
+				"load mmc 0 ${splashimage} ${prefix}boot.bmp; " \
+				"bmp d ${splashimage}; " \
+			"fi; " \
+		"done\0" \
 	"boot_scripts=boot.scr.uimg boot.scr\0" \
 	"boot_script_dhcp=boot.scr.uimg\0" \
 	BOOTENV_BOOT_TARGETS \
diff --git a/include/configs/sunxi-common.h b/include/configs/sunxi-common.h
index 02d7be0849..cbdea20d08 100644
--- a/include/configs/sunxi-common.h
+++ b/include/configs/sunxi-common.h
@@ -284,6 +284,16 @@ extern int soft_i2c_gpio_scl;
 
 #endif /* CONFIG_VIDEO */
 
+#if defined CONFIG_VIDEO || defined CONFIG_DM_VIDEO
+#define CONFIG_VIDEO_LOGO
+#define CONFIG_SPLASH_SCREEN
+#define CONFIG_SPLASH_SCREEN_ALIGN
+#define CONFIG_BMP_16BPP
+#define CONFIG_BMP_24BPP
+#define CONFIG_BMP_32BPP
+#define CONFIG_VIDEO_BMP_RLE8
+#endif
+
 /* Ethernet support */
 #ifdef CONFIG_SUNXI_EMAC
 #define CONFIG_PHY_ADDR		1
@@ -444,7 +454,7 @@ extern int soft_i2c_gpio_scl;
 
 #ifdef CONFIG_USB_KEYBOARD
 #define CONSOLE_STDIN_SETTINGS \
-	"preboot=usb start\0" \
+	"preboot=run loadsplash; usb start\0" \
 	"stdin=serial,usbkbd\0"
 #else
 #define CONSOLE_STDIN_SETTINGS \
