diff --git a/arch/arm/dts/Makefile b/arch/arm/dts/Makefile
old mode 100644
new mode 100755
index d1bd78c..f268593
--- a/arch/arm/dts/Makefile
+++ b/arch/arm/dts/Makefile
@@ -317,6 +317,7 @@ dtb-$(CONFIG_MACH_SUN8I_H3) += \
 	sun8i-h3-orangepi-2.dtb \
 	sun8i-h3-orangepi-lite.dtb \
 	sun8i-h3-orangepi-one.dtb \
+	sun8i-h3-beelink-x2.dtb \
 	sun8i-h3-orangepi-pc.dtb \
 	sun8i-h3-orangepi-pc-plus.dtb \
 	sun8i-h3-orangepi-plus.dtb \
diff --git a/arch/arm/dts/sun8i-h3-beelink-x2.dts b/arch/arm/dts/sun8i-h3-beelink-x2.dts
new file mode 100755
index 0000000..515a3da
--- /dev/null
+++ b/arch/arm/dts/sun8i-h3-beelink-x2.dts
@@ -0,0 +1,88 @@
+/*
+ * Copyright (C) 2016 Hans de Goede <hdegoede@redhat.com>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This file is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+/* The Orange Pi PC Plus is an extended version of the regular PC */
+#include "sun8i-h3-orangepi-pc.dts"
+
+/ {
+	model = "Beelink X2";
+	compatible = "xunlong,orangepi-pc-plus", "allwinner,sun8i-h3";
+
+	aliases {
+		/* ethernet0 is the H3 emac, defined in sun8i-h3.dtsi */
+		ethernet1 = &rtl8189ftv;
+	};
+};
+
+&mmc1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc1_pins_a>;
+	vmmc-supply = <&reg_vcc3v3>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+
+	/*
+	 * Explicitly define the sdio device, so that we can add an ethernet
+	 * alias for it (which e.g. makes u-boot set a mac-address).
+	 */
+	rtl8189ftv: sdio_wifi@1 {
+		reg = <1>;
+	};
+};
+
+&mmc2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc2_8bit_pins>;
+	vmmc-supply = <&reg_vcc3v3>;
+	bus-width = <8>;
+	non-removable;
+	cap-mmc-hw-reset;
+	status = "okay";
+};
+
+&mmc2_8bit_pins {
+	/* Increase drive strength for DDR modes */
+	allwinner,drive = <SUN4I_PINCTRL_40_MA>;
+	/* eMMC is missing pull-ups */
+	allwinner,pull = <SUN4I_PINCTRL_PULL_UP>;
+};
diff --git a/configs/beelink_x2_defconfig b/configs/beelink_x2_defconfig
new file mode 100755
index 0000000..098fc05
--- /dev/null
+++ b/configs/beelink_x2_defconfig
@@ -0,0 +1,21 @@
+CONFIG_ARM=y
+CONFIG_ARCH_SUNXI=y
+CONFIG_MACH_SUN8I_H3=y
+CONFIG_DRAM_CLK=624
+CONFIG_DRAM_ZQ=3881979
+CONFIG_DRAM_ODT_EN=y
+CONFIG_MMC_SUNXI_SLOT_EXTRA=2
+CONFIG_DEFAULT_DEVICE_TREE="sun8i-h3-beelink-x2"
+# CONFIG_SYS_MALLOC_CLEAR_ON_INIT is not set
+CONFIG_SPL=y
+CONFIG_SPL_I2C_SUPPORT=y
+# CONFIG_CMD_IMLS is not set
+# CONFIG_CMD_FLASH is not set
+# CONFIG_CMD_FPGA is not set
+# CONFIG_SPL_DOS_PARTITION is not set
+# CONFIG_SPL_ISO_PARTITION is not set
+# CONFIG_SPL_EFI_PARTITION is not set
+CONFIG_SUN8I_EMAC=y
+CONFIG_SY8106A_POWER=y
+CONFIG_USB_EHCI_HCD=y
+CONFIG_SYS_USB_EVENT_POLL_VIA_INT_QUEUE=y
