diff --git a/arch/arm/boot/dts/sunxi-h3-h5.dtsi b/arch/arm/boot/dts/sunxi-h3-h5.dtsi
index 11240a83..ccde3a00 100644
--- a/arch/arm/boot/dts/sunxi-h3-h5.dtsi
+++ b/arch/arm/boot/dts/sunxi-h3-h5.dtsi
@@ -40,9 +40,11 @@
  *     OTHER DEALINGS IN THE SOFTWARE.
  */
 
+#include <dt-bindings/clock/sun8i-de2.h>
 #include <dt-bindings/clock/sun8i-h3-ccu.h>
 #include <dt-bindings/clock/sun8i-r-ccu.h>
 #include <dt-bindings/interrupt-controller/arm-gic.h>
+#include <dt-bindings/reset/sun8i-de2.h>
 #include <dt-bindings/reset/sun8i-h3-ccu.h>
 #include <dt-bindings/reset/sun8i-r-ccu.h>
 
@@ -79,12 +81,98 @@
 		};
 	};
 
+	de: display-engine {
+		compatible = "allwinner,sun8i-h3-display-engine";
+		allwinner,pipelines = <&mixer0>,
+				      <&mixer1>;
+		status = "disabled";
+	};
+
 	soc {
 		compatible = "simple-bus";
 		#address-cells = <1>;
 		#size-cells = <1>;
 		ranges;
 
+		display_clocks: clock@1000000 {
+			/* compatible is in per SoC .dtsi file */
+			reg = <0x01000000 0x100000>;
+			clocks = <&ccu CLK_BUS_DE>,
+				 <&ccu CLK_DE>;
+			clock-names = "bus",
+				      "mod";
+			resets = <&ccu RST_BUS_DE>;
+			#clock-cells = <1>;
+			#reset-cells = <1>;
+			assigned-clocks = <&ccu CLK_DE>;
+			assigned-clock-parents = <&ccu CLK_PLL_DE>;
+			assigned-clock-rates = <432000000>;
+		};
+
+		mixer0: mixer@1100000 {
+			compatible = "allwinner,sun8i-h3-de2-mixer0";
+			reg = <0x01100000 0x100000>;
+			clocks = <&display_clocks CLK_BUS_MIXER0>,
+				 <&display_clocks CLK_MIXER0>;
+			clock-names = "bus",
+				      "mod";
+			resets = <&display_clocks RST_MIXER0>;
+			status = "disabled";
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				mixer0_out: port@1 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <1>;
+
+					mixer0_out_tcon0: endpoint@0 {
+						reg = <0>;
+						remote-endpoint = <&tcon0_in_mixer0>;
+					};
+
+					mixer0_out_tcon1: endpoint@1 {
+						reg = <1>;
+						remote-endpoint = <&tcon1_in_mixer0>;
+					};
+				};
+			};
+		};
+
+		mixer1: mixer@1200000 {
+			compatible = "allwinner,sun8i-h3-de2-mixer1";
+			reg = <0x01200000 0x100000>;
+			clocks = <&display_clocks CLK_BUS_MIXER1>,
+				 <&display_clocks CLK_MIXER1>;
+			clock-names = "bus",
+				      "mod";
+			/* resets is in per SoC .dtsi file */
+			status = "disabled";
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				mixer1_out: port@1 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <1>;
+
+					mixer1_out_tcon0: endpoint@0 {
+						reg = <0>;
+						remote-endpoint = <&tcon0_in_mixer1>;
+					};
+
+					mixer1_out_tcon1: endpoint@1 {
+						reg = <1>;
+						remote-endpoint = <&tcon1_in_mixer1>;
+					};
+				};
+			};
+		};
+
 		syscon: syscon@1c00000 {
 			compatible = "allwinner,sun8i-h3-system-controller",
 				"syscon";
@@ -100,6 +188,86 @@
 			#dma-cells = <1>;
 		};
 
+		tcon0: lcd-controller@1c0c000 {
+			compatible = "allwinner,sun8i-h3-tcon";
+			reg = <0x01c0c000 0x1000>;
+			interrupts = <GIC_SPI 86 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_TCON0>,
+				 <&ccu CLK_TCON0>;
+			clock-names = "ahb",
+				      "tcon-ch1";
+			resets = <&ccu RST_BUS_TCON0>;
+			reset-names = "lcd";
+			status = "disabled";
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				tcon0_in: port@0 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <0>;
+
+					tcon0_in_mixer0: endpoint@0 {
+						reg = <0>;
+						remote-endpoint = <&mixer0_out_tcon0>;
+					};
+
+					tcon0_in_mixer1: endpoint@1 {
+						reg = <1>;
+						remote-endpoint = <&mixer1_out_tcon0>;
+					};
+				};
+
+				tcon0_out: port@1 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <1>;
+				};
+			};
+		};
+
+		tcon1: lcd-controller@1c0d000 {
+			compatible = "allwinner,sun8i-h3-tcon";
+			reg = <0x01c0d000 0x1000>;
+			interrupts = <GIC_SPI 87 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_TCON1>,
+				 <&ccu CLK_TVE>;
+			clock-names = "ahb",
+				      "tcon-ch1";
+			resets = <&ccu RST_BUS_TCON1>;
+			reset-names = "lcd";
+			status = "disabled";
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				tcon1_in: port@0 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <0>;
+
+					tcon1_in_mixer0: endpoint@0 {
+						reg = <0>;
+						remote-endpoint = <&mixer0_out_tcon1>;
+					};
+
+					tcon1_in_mixer1: endpoint@1 {
+						reg = <1>;
+						remote-endpoint = <&mixer1_out_tcon1>;
+					};
+				};
+
+				tcon1_out: port@1 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <1>;
+				};
+			};
+		};
+
 		mmc0: mmc@01c0f000 {
 			/* compatible and clocks are in per SoC .dtsi file */
 			reg = <0x01c0f000 0x1000>;
