diff --git a/arch/arm/dts/Makefile b/arch/arm/dts/Makefile
index 9cc5c1e0aa..a3ef6854c2 100644
--- a/arch/arm/dts/Makefile
+++ b/arch/arm/dts/Makefile
@@ -318,6 +318,7 @@ dtb-$(CONFIG_MACH_SUN8I_H3) += \
 	sun8i-h3-orangepi-pc-plus.dtb \
 	sun8i-h3-orangepi-plus.dtb \
 	sun8i-h3-orangepi-plus2e.dtb \
+	sun8i-h3-orangepi-zeroplus2.dtb \
 	sun8i-h3-nanopi-m1.dtb \
 	sun8i-h3-nanopi-m1-plus.dtb \
 	sun8i-h3-nanopi-neo.dtb \
diff --git a/arch/arm/dts/sun8i-h3-orangepi-zeroplus2.dts b/arch/arm/dts/sun8i-h3-orangepi-zeroplus2.dts
new file mode 100644
index 0000000000..b03e3a51a2
--- /dev/null
+++ b/arch/arm/dts/sun8i-h3-orangepi-zeroplus2.dts
@@ -0,0 +1,175 @@
+/*
+ * Copyright (C) 2016 Icenowy Zheng <icenowy@aosc.xyz>
+ *
+ * Based on sun8i-h3-orangepi-one.dts, which is:
+ *   Copyright (C) 2016 Hans de Goede <hdegoede@redhat.com>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This file is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+/dts-v1/;
+#include "sun8i-h3.dtsi"
+#include "sunxi-common-regulators.dtsi"
+
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/input/input.h>
+#include <dt-bindings/pinctrl/sun4i-a10.h>
+
+/ {
+	model = "Xunlong Orange Pi Zero Plus 2";
+	compatible = "xunlong,orangepi-zeroplus", "allwinner,sun8i-h3";
+
+	aliases {
+		serial0 = &uart0;
+		/* ethernet0 is the H3 emac, defined in sun8i-h3.dtsi */
+		ethernet1 = &brcmf;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		pwr_led {
+			label = "orangepi:green:pwr";
+			gpios = <&r_pio 0 10 GPIO_ACTIVE_HIGH>;
+			default-state = "on";
+		};
+
+		status_led {
+			label = "orangepi:red:status";
+			gpios = <&pio 0 17 GPIO_ACTIVE_HIGH>;
+		};
+	};
+
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		pinctrl-names = "default";
+		reset-gpios = <&pio 0 9 GPIO_ACTIVE_LOW>;
+		post-power-on-delay-ms = <50>;
+	};
+};
+
+&ehci1 {
+	status = "okay";
+};
+
+&ehci2 {
+	status = "okay";
+};
+
+&ehci3 {
+	status = "okay";
+};
+
+&emac {
+	phy = <&phy1>;
+	phy-mode = "mii";
+	allwinner,use-internal-phy;
+	allwinner,leds-active-low;
+	status = "okay";
+	phy1: ethernet-phy@1 {
+		reg = <1>;
+	};
+};
+
+&mmc0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc0_pins_a>;
+	vmmc-supply = <&reg_vcc3v3>;
+	bus-width = <4>;
+	cd-gpios = <&pio 5 6 GPIO_ACTIVE_HIGH>; /* PF6 */
+	cd-inverted;
+	status = "okay";
+};
+
+&mmc1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc1_pins_a>;
+	vmmc-supply = <&reg_vcc3v3>;
+	vqmmc-supply = <&reg_vcc3v3>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+
+	brcmf: bcrmf@1 {
+		reg = <1>;
+		compatible = "brcm,bcm4329-fmac";
+		interrupt-parent = <&r_pio>;
+		interrupts = <0 7 IRQ_TYPE_LEVEL_LOW>; /* PL7 / EINT7 */
+		interrupt-names = "host-wake";
+	};
+};
+
+&mmc2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc2_8bit_pins>;
+	vmmc-supply = <&reg_vcc3v3>;
+	bus-width = <8>;
+	non-removable;
+	cap-mmc-hw-reset;
+	status = "okay";
+};
+
+&ohci1 {
+	status = "okay";
+};
+
+&ohci2 {
+	status = "okay";
+};
+
+&ohci3 {
+	status = "okay";
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_pins_a>;
+	status = "okay";
+};
+
+&usbphy {
+	/* USB VBUS is always on */
+	status = "okay";
+};
+
diff --git a/configs/orangepi_zero_plus2_h3_defconfig b/configs/orangepi_zero_plus2_h3_defconfig
new file mode 100644
index 0000000000..9257b7c1ed
--- /dev/null
+++ b/configs/orangepi_zero_plus2_h3_defconfig
@@ -0,0 +1,19 @@
+CONFIG_ARM=y
+CONFIG_ARCH_SUNXI=y
+CONFIG_MACH_SUN8I_H3=y
+CONFIG_DRAM_CLK=408
+CONFIG_DRAM_ZQ=3881979
+CONFIG_DRAM_ODT_EN=y
+CONFIG_DEFAULT_DEVICE_TREE="sun8i-h3-orangepi-zeroplus2"
+CONFIG_MMC_SUNXI_SLOT_EXTRA=2
+# CONFIG_SYS_MALLOC_CLEAR_ON_INIT is not set
+CONFIG_SPL=y
+CONFIG_SPL_SPI_FLASH_SUPPORT=y
+CONFIG_SPL_SPI_SUNXI=y
+# CONFIG_CMD_IMLS is not set
+# CONFIG_CMD_FLASH is not set
+# CONFIG_CMD_FPGA is not set
+# CONFIG_SPL_DOS_PARTITION is not set
+# CONFIG_SPL_ISO_PARTITION is not set
+# CONFIG_SPL_EFI_PARTITION is not set
+CONFIG_USB_EHCI_HCD=y
