diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus2.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus2.dts
index b6b7a561..a42fd79a 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus2.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus2.dts
@@ -71,7 +71,7 @@
 	pinctrl-0 = <&mmc0_pins_a>, <&mmc0_cd_pin>;
 	vmmc-supply = <&reg_vcc3v3>;
 	bus-width = <4>;
-	cd-gpios = <&pio 5 6 GPIO_ACTIVE_HIGH>;
+	cd-gpios = <&pio 5 6 GPIO_ACTIVE_LOW>;
 	status = "okay";
 };
 
