diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-orangepi-win.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-orangepi-win.dts
index 5f8ff40..6ecb700 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-orangepi-win.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-orangepi-win.dts
@@ -64,6 +64,27 @@
 		regulator-min-microvolt = <3300000>;
 		regulator-max-microvolt = <3300000>;
 	};
+
+	reg_usb1_vbus: usb1-vbus {
+		compatible = "regulator-fixed";
+		regulator-name = "usb1-vbus";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		regulator-boot-on;
+		enable-active-high;
+		gpio = <&pio 3 7 GPIO_ACTIVE_HIGH>;
+		status = "okay";
+	};
+
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		reset-gpios = <&r_pio 0 8 GPIO_ACTIVE_LOW>; /* PL8 */
+		post-power-on-delay-ms = <50>;
+	};
+};
+
+&ehci0 {
+	status = "okay";
 };
 
 &ehci1 {
@@ -79,10 +100,154 @@
 	status = "okay";
 };
 
+&mmc1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc1_pins>;
+	vmmc-supply = <&reg_dldo2>;
+	vqmmc-supply = <&reg_dldo4>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+
+	brcmf: brcmf@1 {
+		reg = <1>;
+		compatible = "brcm,bcm4329-fmac";
+		interrupt-parent = <&r_pio>;
+		interrupts = <0 7 IRQ_TYPE_LEVEL_LOW>; /* PL7 / EINT7 */
+		interrupt-names = "host-wake";
+	};
+};
+
+&ohci0 {
+	status = "okay";
+};
+
 &ohci1 {
 	status = "okay";
 };
 
+&r_rsb {
+        status = "okay";
+
+        axp803: pmic@3a3 {
+                compatible = "x-powers,axp803";
+                reg = <0x3a3>;
+                interrupt-parent = <&nmi_intc>;
+                interrupts = <0 IRQ_TYPE_LEVEL_LOW>;
+        };
+};
+
+#include <arm/axp803.dtsi>
+
+&reg_aldo1 {
+	regulator-min-microvolt = <2800000>;
+	regulator-max-microvolt = <2800000>;
+	regulator-name = "vcc-csi";
+};
+
+&reg_aldo2 {
+	regulator-always-on;
+	regulator-min-microvolt = <1800000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "vcc-pl";
+};
+
+&reg_aldo3 {
+	regulator-always-on;
+	regulator-min-microvolt = <2700000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "vcc-pll-avcc";
+};
+
+&reg_dc1sw {
+	regulator-always-on;
+	regulator-name = "vcc-phy";
+};
+
+&reg_dcdc1 {
+	regulator-always-on;
+	regulator-min-microvolt = <3300000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "vcc-3v3";
+};
+
+&reg_dcdc2 {
+	regulator-always-on;
+	regulator-min-microvolt = <1000000>;
+	regulator-max-microvolt = <1300000>;
+	regulator-name = "vdd-cpux";
+};
+
+/* DCDC3 is polyphased with DCDC2 */
+
+&reg_dcdc5 {
+	regulator-always-on;
+	regulator-min-microvolt = <1500000>;
+	regulator-max-microvolt = <1500000>;
+	regulator-name = "vcc-dram";
+};
+
+&reg_dcdc6 {
+	regulator-always-on;
+	regulator-min-microvolt = <1100000>;
+	regulator-max-microvolt = <1100000>;
+	regulator-name = "vdd-sys";
+};
+
+&reg_dldo1 {
+	regulator-min-microvolt = <3300000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "vcc-hdmi";
+};
+
+&reg_dldo2 {
+	regulator-min-microvolt = <3300000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "vcc-mipi";
+};
+
+&reg_dldo3 {
+	regulator-min-microvolt = <3300000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "avdd-csi";
+};
+
+&reg_dldo4 {
+	regulator-min-microvolt = <3300000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "vcc-wifi";
+};
+
+&reg_eldo1 {
+	regulator-min-microvolt = <1800000>;
+	regulator-max-microvolt = <1800000>;
+	regulator-name = "cpvdd";
+};
+
+&reg_eldo3 {
+	regulator-min-microvolt = <1800000>;
+	regulator-max-microvolt = <1800000>;
+	regulator-name = "vdd-1v8-csi";
+};
+
+&reg_fldo1 {
+	regulator-min-microvolt = <1200000>;
+	regulator-max-microvolt = <1200000>;
+	regulator-name = "vcc-1v2-hsic";
+};
+
+&reg_fldo2 {
+	regulator-always-on;
+	regulator-min-microvolt = <1100000>;
+	regulator-max-microvolt = <1100000>;
+	regulator-name = "vdd-cpus";
+};
+
+&reg_rtc_ldo {
+	regulator-name = "vcc-rtc";
+};
+
 &uart0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart0_pins_a>;
@@ -90,6 +255,7 @@
 };
 
 &usbphy {
+	usb1_vbus-supply = <&reg_usb1_vbus>;
 	status = "okay";
 };
 
