diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
index 68aadc9..912bb06 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
@@ -325,6 +325,16 @@
 				drive-strength = <40>;
 			};
 
+			spi0_pins: spi0 {
+				pins = "PC0", "PC1", "PC2", "PC3";
+				function = "spi0";
+			};
+
+			spi1_pins: spi1 {
+				pins = "PA15", "PA16", "PA14", "PA13";
+				function = "spi1";
+			};
+
 			uart0_pins_a: uart0@0 {
 				pins = "PB8", "PB9";
 				function = "uart0";
@@ -361,6 +371,34 @@
 			};
 		};
 
+		spi0: spi@01c68000 {
+			compatible = "allwinner,sun8i-h3-spi";
+			reg = <0x01c68000 0x1000>;
+			interrupts = <GIC_SPI 65 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_SPI0>, <&ccu CLK_SPI0>;
+			clock-names = "ahb", "mod";
+			pinctrl-names = "default";
+			pinctrl-0 = <&spi0_pins>;
+			resets = <&ccu RST_BUS_SPI0>;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		spi1: spi@01c69000 {
+			compatible = "allwinner,sun8i-h3-spi";
+			reg = <0x01c69000 0x1000>;
+			interrupts = <GIC_SPI 66 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_SPI1>, <&ccu CLK_SPI1>;
+			clock-names = "ahb", "mod";
+			pinctrl-names = "default";
+			pinctrl-0 = <&spi1_pins>;
+			resets = <&ccu RST_BUS_SPI1>;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
 		uart0: serial@1c28000 {
 			compatible = "snps,dw-apb-uart";
 			reg = <0x01c28000 0x400>;
