diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi
index d9a720bf..55b95569 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi
@@ -76,6 +76,23 @@
 		};
 	};
 
+	iio-hwmon {
+		compatible = "iio-hwmon";
+		io-channels = <&ths>;
+	};
+
+	soc {
+		ths: thermal-sensor@1c25000 {
+			compatible = "allwinner,sun50i-h5-ths";
+			reg = <0x01c25000 0x100>;
+			clocks = <&ccu CLK_BUS_THS>, <&ccu CLK_THS>;
+			clock-names = "bus", "mod";
+			resets = <&ccu RST_BUS_THS>;
+			#thermal-sensor-cells = <0>;
+			#io-channel-cells = <0>;
+		};
+	};
+
 	psci {
 		compatible = "arm,psci-0.2";
 		method = "smc";
