From cef44d8fd32cf32dc3760ba2cf520467df7585d6 Mon Sep 17 00:00:00 2001
From: Sebastian Panceac <sebastian@resin.io>
Date: Wed, 20 Jun 2018 11:15:30 +0200
Subject: [PATCH] Enable i2c0 on OrangePi Plus2 board

Upstream-Status: Inappropriate [configuration]
Signed-off-by: Sebastian Panceac <sebastian@resin.io>
---
 arch/arm/boot/dts/sun8i-h3-orangepi-plus.dts | 4 ++++
 1 file changed, 4 insertions(+)

diff --git a/arch/arm/boot/dts/sun8i-h3-orangepi-plus.dts b/arch/arm/boot/dts/sun8i-h3-orangepi-plus.dts
index b403e5d..781b6c4 100644
--- a/arch/arm/boot/dts/sun8i-h3-orangepi-plus.dts
+++ b/arch/arm/boot/dts/sun8i-h3-orangepi-plus.dts
@@ -122,3 +122,7 @@
 &usbphy {
 	usb3_vbus-supply = <&reg_usb3_vbus>;
 };
+
+&i2c0 {
+	status = "okay";
+};
-- 
2.7.4

