diff --git a/arch/arm/boot/dts/sun8i-h3.dtsi b/arch/arm/boot/dts/sun8i-h3.dtsi
index a0cee17fe44b..efe3a8e4f2af 100644
--- a/arch/arm/boot/dts/sun8i-h3.dtsi
+++ b/arch/arm/boot/dts/sun8i-h3.dtsi
@@ -108,6 +108,23 @@
 		};
 	};
 
+	iio-hwmon {
+		compatible = "iio-hwmon";
+		io-channels = <&ths>;
+	};
+
+	soc {
+		ths: thermal-sensor@1c25000 {
+			compatible = "allwinner,sun8i-h3-ths";
+			reg = <0x01c25000 0x100>;
+			clocks = <&ccu CLK_BUS_THS>, <&ccu CLK_THS>;
+			clock-names = "bus", "mod";
+			resets = <&ccu RST_BUS_THS>;
+			#thermal-sensor-cells = <0>;
+			#io-channel-cells = <0>;
+		};
+	};
+
 	timer {
 		compatible = "arm,armv7-timer";
 		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
