From 89f47cc89889248c8747422d45ddfff9d6993aaf Mon Sep 17 00:00:00 2001
From: Icenowy Zheng <icenowy@aosc.io>
Date: Sun, 3 Sep 2017 17:30:46 +0800
Subject: [PATCH] Revert "arm64: dts: allwinner: Revert EMAC changes"

This reverts commit 87e1f5e8bb4bd584de0a8f3b1e42196dca221d02.

Signed-off-by: Icenowy Zheng <icenowy@aosc.io>
---
 .../boot/dts/allwinner/sun50i-a64-bananapi-m64.dts   | 16 ++++++++++++++++
 .../boot/dts/allwinner/sun50i-a64-pine64-plus.dts    | 15 +++++++++++++++
 arch/arm64/boot/dts/allwinner/sun50i-a64-pine64.dts  | 17 +++++++++++++++++
 .../dts/allwinner/sun50i-a64-sopine-baseboard.dts    | 16 ++++++++++++++++
 arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi        | 20 ++++++++++++++++++++
 .../boot/dts/allwinner/sun50i-h5-nanopi-neo2.dts     | 17 +++++++++++++++++
 .../boot/dts/allwinner/sun50i-h5-orangepi-pc2.dts    | 17 +++++++++++++++++
 .../boot/dts/allwinner/sun50i-h5-orangepi-prime.dts  | 17 +++++++++++++++++
 8 files changed, 135 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-bananapi-m64.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-bananapi-m64.dts
index 6872135d7f849..ba2fde2909f94 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-bananapi-m64.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-bananapi-m64.dts
@@ -51,6 +51,7 @@
 	compatible = "sinovoip,bananapi-m64", "allwinner,sun50i-a64";
 
 	aliases {
+		ethernet0 = &emac;
 		serial0 = &uart0;
 		serial1 = &uart1;
 	};
@@ -67,6 +68,14 @@
 	};
 };
 
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&rgmii_pins>;
+	phy-mode = "rgmii";
+	phy-handle = <&ext_rgmii_phy>;
+	status = "okay";
+};
+
 &i2c1 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&i2c1_pins>;
@@ -77,6 +86,13 @@
 	bias-pull-up;
 };
 
+&mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
+};
+
 &mmc0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc0_pins>;
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pine64-plus.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-pine64-plus.dts
index f82ccf332c0fa..24f1aac366d64 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pine64-plus.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pine64-plus.dts
@@ -48,3 +48,18 @@
 
 	/* TODO: Camera, touchscreen, etc. */
 };
+
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&rgmii_pins>;
+	phy-mode = "rgmii";
+	phy-handle = <&ext_rgmii_phy>;
+	status = "okay";
+};
+
+&mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
+};
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-pine64.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-pine64.dts
index 7c533b6d4ba9a..827168bc22ed2 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-pine64.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-pine64.dts
@@ -51,6 +51,7 @@
 	compatible = "pine64,pine64", "allwinner,sun50i-a64";
 
 	aliases {
+		ethernet0 = &emac;
 		serial0 = &uart0;
 		serial1 = &uart1;
 		serial2 = &uart2;
@@ -78,6 +79,15 @@
 	status = "okay";
 };
 
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&rmii_pins>;
+	phy-mode = "rmii";
+	phy-handle = <&ext_rmii_phy1>;
+	status = "okay";
+
+};
+
 &i2c1 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&i2c1_pins>;
@@ -88,6 +98,13 @@
 	bias-pull-up;
 };
 
+&mdio {
+	ext_rmii_phy1: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
+};
+
 &mmc0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc0_pins>;
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-sopine-baseboard.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-sopine-baseboard.dts
index d891a1a27f6c5..216e3a5dafaef 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-sopine-baseboard.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-sopine-baseboard.dts
@@ -53,6 +53,7 @@
 		     "allwinner,sun50i-a64";
 
 	aliases {
+		ethernet0 = &emac;
 		serial0 = &uart0;
 	};
 
@@ -76,6 +77,21 @@
 	status = "okay";
 };
 
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&rgmii_pins>;
+	phy-mode = "rgmii";
+	phy-handle = <&ext_rgmii_phy>;
+	status = "okay";
+};
+
+&mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
+};
+
 &mmc2 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc2_pins>;
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
index 68aadc9b96dc1..bd0f33b77f572 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
@@ -449,6 +449,26 @@
 			#size-cells = <0>;
 		};
 
+		emac: ethernet@1c30000 {
+			compatible = "allwinner,sun50i-a64-emac";
+			syscon = <&syscon>;
+			reg = <0x01c30000 0x10000>;
+			interrupts = <GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "macirq";
+			resets = <&ccu RST_BUS_EMAC>;
+			reset-names = "stmmaceth";
+			clocks = <&ccu CLK_BUS_EMAC>;
+			clock-names = "stmmaceth";
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+
+			mdio: mdio {
+				#address-cells = <1>;
+				#size-cells = <0>;
+			};
+		};
+
 		gic: interrupt-controller@1c81000 {
 			compatible = "arm,gic-400";
 			reg = <0x01c81000 0x1000>,
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo2.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo2.dts
index 1c2387bd5df6f..9689087611945 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo2.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-nanopi-neo2.dts
@@ -50,6 +50,7 @@
 	compatible = "friendlyarm,nanopi-neo2", "allwinner,sun50i-h5";
 
 	aliases {
+		ethernet0 = &emac;
 		serial0 = &uart0;
 	};
 
@@ -108,6 +109,22 @@
 	status = "okay";
 };
 
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_gmac_3v3>;
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii";
+	status = "okay";
+};
+
+&external_mdio {
+	ext_rgmii_phy: ethernet-phy@7 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <7>;
+	};
+};
+
 &mmc0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc0_pins_a>, <&mmc0_cd_pin>;
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-pc2.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-pc2.dts
index 4f77c8470f6c3..a8296feee8841 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-pc2.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-pc2.dts
@@ -59,6 +59,7 @@
 	};
 
 	aliases {
+		ethernet0 = &emac;
 		serial0 = &uart0;
 	};
 
@@ -136,12 +137,28 @@
 	status = "okay";
 };
 
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_gmac_3v3>;
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii";
+	status = "okay";
+};
+
 &ir {
 	pinctrl-names = "default";
 	pinctrl-0 = <&ir_pins_a>;
 	status = "okay";
 };

+&external_mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
+};
+
 &mmc0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc0_pins_a>, <&mmc0_cd_pin>;
diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-prime.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-prime.dts
index 6be06873e5afe..d906b302cbcdc 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-prime.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-prime.dts
@@ -54,6 +54,7 @@
 	compatible = "xunlong,orangepi-prime", "allwinner,sun50i-h5";
 
 	aliases {
+		ethernet0 = &emac;
 		serial0 = &uart0;
 	};
 
@@ -143,12 +144,28 @@
 	status = "okay";
 };
 
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_gmac_3v3>;
+	phy-handle = <&ext_rgmii_phy>;
+	phy-mode = "rgmii";
+	status = "okay";
+};
+
 &ir {
 	pinctrl-names = "default";
 	pinctrl-0 = <&ir_pins_a>;
 	status = "okay";
 };

+&external_mdio {
+	ext_rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
+};
+
 &mmc0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc0_pins_a>, <&mmc0_cd_pin>;
