diff --git a/arch/arm/boot/dts/Makefile b/arch/arm/boot/dts/Makefile
index 4b17f35d..6a6639ab 100644
--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -918,6 +918,7 @@ dtb-$(CONFIG_MACH_SUN8I) += \
 	sun8i-h3-orangepi-pc-plus.dtb \
 	sun8i-h3-orangepi-plus.dtb \
 	sun8i-h3-orangepi-plus2e.dtb \
+	sun8i-h3-orangepi-zeroplus2.dtb \
	sun8i-r16-bananapi-m2m.dtb \
	sun8i-r16-parrot.dtb \
	sun8i-v3s-licheepi-zero.dtb \
diff --git a/arch/arm/boot/dts/sun8i-h3-orangepi-zeroplus2.dts b/arch/arm/boot/dts/sun8i-h3-orangepi-zeroplus2.dts
new file mode 100644
index 0000000..9856052
--- /dev/null
+++ b/arch/arm/boot/dts/sun8i-h3-orangepi-zeroplus2.dts
@@ -0,0 +1,229 @@
+/*
+ * Copyright (C) Armbian
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This file is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+/dts-v1/;
+#include "sun8i-h3.dtsi"
+#include "sunxi-common-regulators.dtsi"
+#include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/input/input.h>
+
+/ {
+	model = "Xunlong Orange Pi Zero Plus 2";
+	compatible = "xunlong,orangepi-zeroplus", "allwinner,sun8i-h3";
+
+	aliases {
+		ethernet1 = &brcmf;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		pwr_led {
+			label = "orangepi:green:pwr";
+			gpios = <&r_pio 0 10 GPIO_ACTIVE_HIGH>;
+			default-state = "on";
+		};
+
+		status_led {
+			label = "orangepi:red:status";
+			gpios = <&pio 0 17 GPIO_ACTIVE_HIGH>;
+			linux,default-trigger = "heartbeat";
+		};
+	};
+
+	connector {
+		compatible = "hdmi-connector";
+		type = "a";
+
+		port {
+			hdmi_con_in: endpoint {
+				remote-endpoint = <&hdmi_out_con>;
+			};
+		};
+	};
+
+	/delete-node/ reg_vcc_wifi;
+
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		reset-gpios = <&pio 0 9 GPIO_ACTIVE_LOW>;
+		post-power-on-delay-ms = <50>;
+	};
+
+	reg_usb1_vbus: usb1-vbus {
+		/delete-property/ gpio;
+		gpio = <&pio 3 6 GPIO_ACTIVE_HIGH>;
+		status = "okay";
+	};
+
+};
+
+&de {
+	status = "okay";
+};
+
+&ehci0 {
+	status = "okay";
+};
+
+
+&hdmi {
+	status = "okay";
+};
+
+&hdmi_out {
+	hdmi_out_con: endpoint {
+		remote-endpoint = <&hdmi_con_in>;
+	};
+};
+
+&sound_hdmi {
+	status = "okay";
+};
+
+&i2s2 {
+	status = "okay";
+};
+
+&mixer0 {
+	status = "okay";
+};
+
+&tcon0 {
+	status = "okay";
+};
+
+&mmc0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc0_pins_a>;
+	vmmc-supply = <&reg_vcc3v3>;
+	bus-width = <4>;
+	cd-gpios = <&pio 5 6 GPIO_ACTIVE_HIGH>; /* PF6 */
+	cd-inverted;
+	status = "okay";
+};
+
+&mmc1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc1_pins_a>;
+	vmmc-supply = <&reg_vcc3v3>;
+	vqmmc-supply = <&reg_vcc3v3>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+
+	/delete-node/ sdio_wifi@1;
+
+	brcmf: bcrmf@1 {
+		reg = <1>;
+		compatible = "brcm,bcm4329-fmac";
+		interrupt-parent = <&r_pio>;
+		interrupts = <0 7 IRQ_TYPE_LEVEL_LOW>; /* PL7 / EINT7 */
+		interrupt-names = "host-wake";
+	};
+};
+
+&mmc2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc2_8bit_pins>;
+	vmmc-supply = <&reg_vcc3v3>;
+	bus-width = <8>;
+	non-removable;
+	cap-mmc-hw-reset;
+	status = "okay";
+};
+
+&pio {
+    bt_pwr_pin: bt_pwr_pin@0 {
+        pins = "PA10";
+        function = "gpio_out";
+    };
+};
+
+&ohci0 {
+	status = "okay";
+};
+
+&spi0 {
+	/* Disable SPI NOR by default: it optional on Orange Pi Zero boards */
+	status = "disabled";
+
+	flash@0 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "mxicy,mx25l1606e", "winbond,w25q128";
+		reg = <0>;
+		spi-max-frequency = <40000000>;
+	};
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_pins_a>;
+	status = "okay";
+};
+
+&uart1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart1_pins>, <&uart1_rts_cts_pins>;
+	status = "okay";
+};
+
+&usb_otg {
+	dr_mode = "peripheral";
+	status = "okay";
+};
+
+&usbphy {
+	/*
+	 * USB Type-A port VBUS is always on. However, MicroUSB VBUS can only
+	 * power up the board; when it's used as OTG port, this VBUS is
+	 * always off even if the board is powered via GPIO pins.
+	 */
+	status = "okay";
+	usb0_id_det-gpios = <&pio 6 12 GPIO_ACTIVE_HIGH>; /* PG12 */
+};
