diff --git a/arch/arm/boot/dts/sun8i-h3.dtsi b/arch/arm/boot/dts/sun8i-h3.dtsi
index b36f9f42..f2973669 100644
--- a/arch/arm/boot/dts/sun8i-h3.dtsi
+++ b/arch/arm/boot/dts/sun8i-h3.dtsi
@@ -72,6 +72,49 @@
 		};
 	};
 
+	soc {
+		mali: gpu@1c40000 {
+			compatible = "allwinner,sun8i-h3-mali",
+				     "allwinner,sun7i-a20-mali", "arm,mali-400";
+			reg = <0x01c40000 0x10000>;
+			interrupts = <GIC_SPI 97 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 98 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 99 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 100 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 102 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 103 IRQ_TYPE_LEVEL_HIGH>,
+				     <GIC_SPI 101 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "gp",
+					  "gpmmu",
+					  "pp0",
+					  "ppmmu0",
+					  "pp1",
+					  "ppmmu1",
+					  "pmu";
+			clocks = <&ccu CLK_BUS_GPU>, <&ccu CLK_GPU>;
+			clock-names = "bus", "core";
+			resets = <&ccu RST_BUS_GPU>;
+			memory-region = <&cma>;
+
+			assigned-clocks = <&ccu CLK_GPU>;
+			assigned-clock-rates = <384000000>;
+		};
+	};
+
+	reserved-memory {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		ranges;
+
+		cma: linux,cma {
+			compatible = "shared-dma-pool";
+			reusable;
+			size = <0x4000000>;
+			alignment = <0x2000>;
+			linux,cma-default;
+		};
+	};
+
 	timer {
 		compatible = "arm,armv7-timer";
 		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
