diff --git a/Documentation/devicetree/bindings/phy/sun4i-usb-phy.txt b/Documentation/devicetree/bindings/phy/sun4i-usb-phy.txt
index cbc7847..0f00abd 100644
--- a/Documentation/devicetree/bindings/phy/sun4i-usb-phy.txt
+++ b/Documentation/devicetree/bindings/phy/sun4i-usb-phy.txt
@@ -11,6 +11,7 @@ Required properties:
   * allwinner,sun8i-a33-usb-phy
   * allwinner,sun8i-a83t-usb-phy
   * allwinner,sun8i-h3-usb-phy
+  * allwinner,sun8i-r40-usb-phy
   * allwinner,sun8i-v3s-usb-phy
   * allwinner,sun50i-a64-usb-phy
 - reg : a list of offset + length pairs
diff --git a/Documentation/devicetree/bindings/sound/sun4i-i2s.txt b/Documentation/devicetree/bindings/sound/sun4i-i2s.txt
index fc5da60..597dcd4 100644
--- a/Documentation/devicetree/bindings/sound/sun4i-i2s.txt
+++ b/Documentation/devicetree/bindings/sound/sun4i-i2s.txt
@@ -8,6 +8,7 @@ Required properties:
 - compatible: should be one of the following:
    - "allwinner,sun4i-a10-i2s"
    - "allwinner,sun6i-a31-i2s"
+   - "allwinner,sun8i-a83t-i2s"
    - "allwinner,sun8i-h3-i2s"
 - reg: physical base address of the controller and length of memory mapped
   region.
@@ -23,6 +24,7 @@ Required properties:
 
 Required properties for the following compatibles:
 	- "allwinner,sun6i-a31-i2s"
+	- "allwinner,sun8i-a83t-i2s"
 	- "allwinner,sun8i-h3-i2s"
 - resets: phandle to the reset line for this codec
 
diff --git a/arch/arm/boot/dts/Makefile b/arch/arm/boot/dts/Makefile
index 6817198..2fd4d80 100644
--- a/arch/arm/boot/dts/Makefile
+++ b/arch/arm/boot/dts/Makefile
@@ -936,6 +936,7 @@ dtb-$(CONFIG_MACH_SUN8I) += \
 	sun8i-h3-orangepi-zeroplus2.dtb \
 	sun8i-r16-bananapi-m2m.dtb \
 	sun8i-r16-parrot.dtb \
+	sun8i-r40-bananapi-m2-ultra.dtb \
 	sun8i-v3s-licheepi-zero.dtb \
 	sun8i-v3s-licheepi-zero-dock.dtb
 dtb-$(CONFIG_MACH_SUN9I) += \
diff --git a/arch/arm/boot/dts/axp81x.dtsi b/arch/arm/boot/dts/axp81x.dtsi
new file mode 100644
index 0000000..73b761f
--- /dev/null
+++ b/arch/arm/boot/dts/axp81x.dtsi
@@ -0,0 +1,139 @@
+/*
+ * Copyright 2017 Chen-Yu Tsai
+ *
+ * Chen-Yu Tsai <wens@csie.org>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This file is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+/* AXP813/818 Integrated Power Management Chip */
+
+&axp81x {
+	interrupt-controller;
+	#interrupt-cells = <1>;
+
+	regulators {
+		/* Default work frequency for buck regulators */
+		x-powers,dcdc-freq = <3000>;
+
+		reg_dcdc1: dcdc1 {
+		};
+
+		reg_dcdc2: dcdc2 {
+		};
+
+		reg_dcdc3: dcdc3 {
+		};
+
+		reg_dcdc4: dcdc4 {
+		};
+
+		reg_dcdc5: dcdc5 {
+		};
+
+		reg_dcdc6: dcdc6 {
+		};
+
+		reg_dcdc7: dcdc7 {
+		};
+
+		reg_aldo1: aldo1 {
+		};
+
+		reg_aldo2: aldo2 {
+		};
+
+		reg_aldo3: aldo3 {
+		};
+
+		reg_dldo1: dldo1 {
+		};
+
+		reg_dldo2: dldo2 {
+		};
+
+		reg_dldo3: dldo3 {
+		};
+
+		reg_dldo4: dldo4 {
+		};
+
+		reg_eldo1: eldo1 {
+		};
+
+		reg_eldo2: eldo2 {
+		};
+
+		reg_eldo3: eldo3 {
+		};
+
+		reg_fldo1: fldo1 {
+		};
+
+		reg_fldo2: fldo2 {
+		};
+
+		reg_fldo3: fldo3 {
+		};
+
+		reg_ldo_io0: ldo-io0 {
+			/* Disable by default to avoid conflicts with GPIO */
+			status = "disabled";
+		};
+
+		reg_ldo_io1: ldo-io1 {
+			/* Disable by default to avoid conflicts with GPIO */
+			status = "disabled";
+		};
+
+		reg_rtc_ldo: rtc-ldo {
+			/* RTC_LDO is a fixed, always-on regulator */
+			regulator-always-on;
+			regulator-min-microvolt = <1800000>;
+			regulator-max-microvolt = <1800000>;
+		};
+
+		reg_sw: sw {
+		};
+
+		reg_drivevbus: drivevbus {
+			status = "disabled";
+		};
+	};
+};
diff --git a/arch/arm/boot/dts/sun8i-a83t-bananapi-m3.dts b/arch/arm/boot/dts/sun8i-a83t-bananapi-m3.dts
old mode 100644
new mode 100755
index 2bafd7e..01a1f29
--- a/arch/arm/boot/dts/sun8i-a83t-bananapi-m3.dts
+++ b/arch/arm/boot/dts/sun8i-a83t-bananapi-m3.dts
@@ -44,7 +44,6 @@
 
 /dts-v1/;
 #include "sun8i-a83t.dtsi"
-#include "sunxi-common-regulators.dtsi"
 
 #include <dt-bindings/gpio/gpio.h>
 
@@ -53,12 +52,41 @@
 	compatible = "sinovoip,bpi-m3", "allwinner,sun8i-a83t";
 
 	aliases {
+		ethernet0 = &emac;
 		serial0 = &uart0;
 	};
 
 	chosen {
 		stdout-path = "serial0:115200n8";
 	};
+
+	reg_vcc3v3: vcc3v3 {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+	};
+
+	reg_usb1_vbus: reg-usb1-vbus {
+		compatible = "regulator-fixed";
+		regulator-name = "usb1-vbus";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		regulator-boot-on;
+		enable-active-high;
+		gpio = <&pio 3 24 GPIO_ACTIVE_HIGH>; /* PD24 */
+	};
+
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		clocks = <&ac100_rtc 1>;
+		clock-names = "ext_clock";
+		/* The WiFi low power clock must be 32768 Hz */
+		assigned-clocks = <&ac100_rtc 1>;
+		assigned-clock-rates = <32768>;
+		/* enables internal regulator and de-asserts reset */
+		reset-gpios = <&r_pio 0 2 GPIO_ACTIVE_LOW>; /* PL2 WL-PMU-EN */
+	};
 };
 
 &ehci0 {
@@ -68,6 +96,24 @@
 	/* TODO GL830 USB-to-SATA bridge downstream w/ GPIO power controls */
 };
 
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_sw>;
+	phy-handle = <&rgmii_phy>;
+	phy-mode = "rgmii";
+	allwinner,rx-delay-ps = <700>;
+	allwinner,tx-delay-ps = <700>;
+	status = "okay";
+};
+
+&mdio {
+	rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
+};
+
 &mmc0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc0_pins>;
@@ -78,6 +124,23 @@
 	status = "okay";
 };
 
+&mmc1 {
+	vmmc-supply = <&reg_dldo1>;
+	vqmmc-supply = <&reg_dldo1>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+
+	brcmf: wifi@1 {
+		reg = <1>;
+		compatible = "brcm,bcm4329-fmac";
+		interrupt-parent = <&r_pio>;
+		interrupts = <0 3 IRQ_TYPE_LEVEL_LOW>;
+		interrupt-names = "host-wake";
+	};
+};
+
 &mmc2 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc2_8bit_emmc_pins>;
@@ -96,6 +159,10 @@
 		reg = <0x3a3>;
 		interrupt-parent = <&r_intc>;
 		interrupts = <0 IRQ_TYPE_LEVEL_LOW>;
+		eldoin-supply = <&reg_dcdc1>;
+		fldoin-supply = <&reg_dcdc5>;
+		swin-supply = <&reg_dcdc1>;
+		x-powers,drive-vbus-en;
 	};
 
 	ac100: codec@e89 {
@@ -123,17 +190,126 @@
 	};
 };
 
-&reg_usb1_vbus {
-	gpio = <&pio 3 24 GPIO_ACTIVE_HIGH>; /* PD24 */
+#include "axp81x.dtsi"
+
+&reg_aldo1 {
+	regulator-always-on;
+	regulator-min-microvolt = <1800000>;
+	regulator-max-microvolt = <1800000>;
+	regulator-name = "vcc-1v8";
+};
+
+&reg_aldo2 {
+	regulator-always-on;
+	regulator-min-microvolt = <1800000>;
+	regulator-max-microvolt = <1800000>;
+	regulator-name = "dram-pll";
+};
+
+&reg_aldo3 {
+	regulator-always-on;
+	regulator-min-microvolt = <3000000>;
+	regulator-max-microvolt = <3000000>;
+	regulator-name = "avcc";
+};
+
+&reg_dcdc1 {
+	/* schematics says 3.1V but FEX file says 3.3V */
+	regulator-always-on;
+	regulator-min-microvolt = <3300000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "vcc-3v3";
+};
+
+&reg_dcdc2 {
+	regulator-always-on;
+	regulator-min-microvolt = <700000>;
+	regulator-max-microvolt = <1100000>;
+	regulator-name = "vdd-cpua";
+};
+
+&reg_dcdc3 {
+	regulator-always-on;
+	regulator-min-microvolt = <700000>;
+	regulator-max-microvolt = <1100000>;
+	regulator-name = "vdd-cpub";
+};
+
+&reg_dcdc4 {
+	regulator-min-microvolt = <700000>;
+	regulator-max-microvolt = <1100000>;
+	regulator-name = "vdd-gpu";
+};
+
+&reg_dcdc5 {
+	regulator-always-on;
+	regulator-min-microvolt = <1200000>;
+	regulator-max-microvolt = <1200000>;
+	regulator-name = "vcc-dram";
+};
+
+&reg_dcdc6 {
+	regulator-always-on;
+	regulator-min-microvolt = <900000>;
+	regulator-max-microvolt = <900000>;
+	regulator-name = "vdd-sys";
+};
+
+&reg_dldo1 {
+	/*
+	 * This powers both the WiFi/BT module's main power, I/O supply,
+	 * and external pull-ups on all the data lines. It should be set
+	 * to the same voltage as the I/O supply (DCDC1 in this case) to
+	 * avoid any leakage or mismatch.
+	 */
+	regulator-min-microvolt = <3300000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "vcc-wifi";
+};
+
+&reg_dldo3 {
+	regulator-always-on;
+	regulator-min-microvolt = <2500000>;
+	regulator-max-microvolt = <2500000>;
+	regulator-name = "vcc-pd";
+};
+
+&reg_drivevbus {
+	regulator-name = "usb0-vbus";
 	status = "okay";
 };
 
-&reg_vcc3v0 {
-	status = "disabled";
+&reg_fldo1 {
+	regulator-min-microvolt = <1080000>;
+	regulator-max-microvolt = <1320000>;
+	regulator-name = "vdd12-hsic";
+};
+
+&reg_fldo2 {
+	/*
+	 * Despite the embedded CPUs core not being used in any way,
+	 * this must remain on or the system will hang.
+	 */
+	regulator-always-on;
+	regulator-min-microvolt = <700000>;
+	regulator-max-microvolt = <1100000>;
+	regulator-name = "vdd-cpus";
+};
+
+&reg_rtc_ldo {
+	regulator-name = "vcc-rtc";
 };
 
-&reg_vcc5v0 {
-	status = "disabled";
+&reg_sw {
+	/*
+	 * The PHY requires 20ms after all voltages
+	 * are applied until core logic is ready and
+	 * 30ms after the reset pin is de-asserted.
+	 * Set a 100ms delay to account for PMIC
+	 * ramp time and board traces.
+	 */
+	regulator-enable-ramp-delay = <100000>;
+	regulator-name = "vcc-ephy";
 };
 
 &uart0 {
diff --git a/arch/arm/boot/dts/sun8i-a83t-cubietruck-plus.dts b/arch/arm/boot/dts/sun8i-a83t-cubietruck-plus.dts
index 716a205..6da08cd 100644
--- a/arch/arm/boot/dts/sun8i-a83t-cubietruck-plus.dts
+++ b/arch/arm/boot/dts/sun8i-a83t-cubietruck-plus.dts
@@ -44,7 +44,6 @@
 
 /dts-v1/;
 #include "sun8i-a83t.dtsi"
-#include "sunxi-common-regulators.dtsi"
 
 #include <dt-bindings/gpio/gpio.h>
 
@@ -53,6 +52,7 @@
 	compatible = "cubietech,cubietruck-plus", "allwinner,sun8i-a83t";
 
 	aliases {
+		ethernet0 = &emac;
 		serial0 = &uart0;
 	};
 
@@ -95,6 +95,26 @@
 		refclk-frequency = <19200000>;
 	};
 
+	reg_usb1_vbus: reg-usb1-vbus {
+		compatible = "regulator-fixed";
+		regulator-name = "usb1-vbus";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		regulator-boot-on;
+		enable-active-high;
+		gpio = <&pio 3 29 GPIO_ACTIVE_HIGH>; /* PD29 */
+	};
+
+	reg_usb2_vbus: reg-usb2-vbus {
+		compatible = "regulator-fixed";
+		regulator-name = "usb2-vbus";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		regulator-boot-on;
+		enable-active-high;
+		gpio = <&r_pio 0 6 GPIO_ACTIVE_HIGH>; /* PL6 */
+	};
+
 	sound {
 		compatible = "simple-audio-card";
 		simple-audio-card,name = "On-board SPDIF";
@@ -112,6 +132,17 @@
 		#sound-dai-cells = <0>;
 		compatible = "linux,spdif-dit";
 	};
+
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		clocks = <&ac100_rtc 1>;
+		clock-names = "ext_clock";
+		/* The WiFi low power clock must be 32768 Hz */
+		assigned-clocks = <&ac100_rtc 1>;
+		assigned-clock-rates = <32768>;
+		/* enables internal regulator and de-asserts reset */
+		reset-gpios = <&r_pio 0 2 GPIO_ACTIVE_LOW>; /* PL2 WL-PMU-EN */
+	};
 };
 
 &ehci0 {
@@ -124,20 +155,45 @@
 	status = "okay";
 };
 
+&emac {
+	pinctrl-names = "default";
+	pinctrl-0 = <&emac_rgmii_pins>;
+	phy-supply = <&reg_dldo4>;
+	phy-handle = <&rgmii_phy>;
+	phy-mode = "rgmii";
+	status = "okay";
+};
+
+&mdio {
+	rgmii_phy: ethernet-phy@1 {
+		compatible = "ethernet-phy-ieee802.3-c22";
+		reg = <1>;
+	};
+};
+
 &mmc0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc0_pins>;
-	vmmc-supply = <&reg_vcc3v3>;
+	vmmc-supply = <&reg_dcdc1>;
 	bus-width = <4>;
 	cd-gpios = <&pio 5 6 GPIO_ACTIVE_HIGH>; /* PF6 */
 	cd-inverted;
 	status = "okay";
 };
 
+&mmc1 {
+	vmmc-supply = <&reg_dcdc1>;
+	vqmmc-supply = <&reg_sw>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+};
+
 &mmc2 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc2_8bit_emmc_pins>;
-	vmmc-supply = <&reg_vcc3v3>;
+	vmmc-supply = <&reg_dcdc1>;
 	bus-width = <8>;
 	non-removable;
 	cap-mmc-hw-reset;
@@ -152,6 +208,9 @@
 		reg = <0x3a3>;
 		interrupt-parent = <&r_intc>;
 		interrupts = <0 IRQ_TYPE_LEVEL_LOW>;
+		eldoin-supply = <&reg_dcdc1>;
+		swin-supply = <&reg_dcdc1>;
+		x-powers,drive-vbus-en;
 	};
 
 	ac100: codec@e89 {
@@ -179,22 +238,143 @@
 	};
 };
 
-&reg_usb1_vbus {
-	gpio = <&pio 3 29 GPIO_ACTIVE_HIGH>; /* PD29 */
-	status = "okay";
+#include "axp81x.dtsi"
+
+&reg_aldo1 {
+	regulator-always-on;
+	regulator-min-microvolt = <1800000>;
+	regulator-max-microvolt = <1800000>;
+	regulator-name = "vcc-1v8";
+};
+
+&reg_aldo2 {
+	regulator-always-on;
+	regulator-min-microvolt = <1800000>;
+	regulator-max-microvolt = <1800000>;
+	regulator-name = "dram-pll";
+};
+
+&reg_aldo3 {
+	regulator-always-on;
+	regulator-min-microvolt = <3000000>;
+	regulator-max-microvolt = <3000000>;
+	regulator-name = "avcc";
+};
+
+&reg_dcdc1 {
+	/*
+	 * The schematics say this should be 3.3V, but the FEX file says
+	 * it should be 3V. The latter makes sense, as the WiFi module's
+	 * I/O is indirectly powered from DCDC1, through SW. It is rated
+	 * at 2.98V maximum.
+	 */
+	regulator-always-on;
+	regulator-min-microvolt = <3000000>;
+	regulator-max-microvolt = <3000000>;
+	regulator-name = "vcc-3v";
+};
+
+&reg_dcdc2 {
+	regulator-always-on;
+	regulator-min-microvolt = <700000>;
+	regulator-max-microvolt = <1100000>;
+	regulator-name = "vdd-cpua";
+};
+
+&reg_dcdc3 {
+	regulator-always-on;
+	regulator-min-microvolt = <700000>;
+	regulator-max-microvolt = <1100000>;
+	regulator-name = "vdd-cpub";
+};
+
+&reg_dcdc4 {
+	regulator-min-microvolt = <700000>;
+	regulator-max-microvolt = <1100000>;
+	regulator-name = "vdd-gpu";
+};
+
+&reg_dcdc5 {
+	regulator-always-on;
+	regulator-min-microvolt = <1500000>;
+	regulator-max-microvolt = <1500000>;
+	regulator-name = "vcc-dram";
+};
+
+&reg_dcdc6 {
+	regulator-always-on;
+	regulator-min-microvolt = <900000>;
+	regulator-max-microvolt = <900000>;
+	regulator-name = "vdd-sys";
+};
+
+&reg_dldo2 {
+	regulator-min-microvolt = <3300000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "dp-pwr";
 };
 
-&reg_usb2_vbus {
-	gpio = <&r_pio 0 6 GPIO_ACTIVE_HIGH>; /* PL6 */
+&reg_dldo3 {
+	regulator-always-on;
+	regulator-min-microvolt = <2500000>;
+	regulator-max-microvolt = <2500000>;
+	regulator-name = "ephy-io";
+};
+
+&reg_dldo4 {
+	/*
+	 * The PHY requires 20ms after all voltages are applied until core
+	 * logic is ready and 30ms after the reset pin is de-asserted.
+	 * Set a 100ms delay to account for PMIC ramp time and board traces.
+	 */
+	regulator-enable-ramp-delay = <100000>;
+	regulator-min-microvolt = <3300000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "ephy";
+};
+
+&reg_drivevbus {
+	regulator-name = "usb0-vbus";
 	status = "okay";
 };
 
-&reg_vcc3v0 {
-	status = "disabled";
+&reg_eldo1 {
+	regulator-min-microvolt = <1200000>;
+	regulator-max-microvolt = <1200000>;
+	regulator-name = "dp-bridge-1";
+};
+
+&reg_eldo2 {
+	regulator-min-microvolt = <1200000>;
+	regulator-max-microvolt = <1200000>;
+	regulator-name = "dp-bridge-2";
+};
+
+&reg_fldo1 {
+	/* TODO should be handled by USB PHY */
+	regulator-always-on;
+	regulator-min-microvolt = <1080000>;
+	regulator-max-microvolt = <1320000>;
+	regulator-name = "vdd12-hsic";
+};
+
+&reg_fldo2 {
+	/*
+	 * Despite the embedded CPUs core not being used in any way,
+	 * this must remain on or the system will hang.
+	 */
+	regulator-always-on;
+	regulator-min-microvolt = <700000>;
+	regulator-max-microvolt = <1100000>;
+	regulator-name = "vdd-cpus";
+};
+
+&reg_rtc_ldo {
+	regulator-name = "vcc-rtc";
 };
 
-&reg_vcc5v0 {
-	status = "disabled";
+&reg_sw {
+	regulator-name = "vcc-wifi-io";
 };
 
 &spdif {
diff --git a/arch/arm/boot/dts/sun8i-a83t.dtsi b/arch/arm/boot/dts/sun8i-a83t.dtsi
index f996bd3..952923a 100644
--- a/arch/arm/boot/dts/sun8i-a83t.dtsi
+++ b/arch/arm/boot/dts/sun8i-a83t.dtsi
@@ -54,12 +54,6 @@
 	#address-cells = <1>;
 	#size-cells = <1>;
 
-	aliases {
-	};
-
-	chosen {
-	};
-
 	cpus {
 		#address-cells = <1>;
 		#size-cells = <0>;
@@ -218,6 +212,8 @@
 			resets = <&ccu RST_BUS_MMC1>;
 			reset-names = "ahb";
 			interrupts = <GIC_SPI 61 IRQ_TYPE_LEVEL_HIGH>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&mmc1_pins>;
 			status = "disabled";
 			#address-cells = <1>;
 			#size-cells = <0>;
@@ -242,7 +238,7 @@
 			#size-cells = <0>;
 		};
 
-		usb_otg: usb@01c19000 {
+		usb_otg: usb@1c19000 {
 			compatible = "allwinner,sun8i-a83t-musb",
 				     "allwinner,sun8i-a33-musb";
 			reg = <0x01c19000 0x0400>;
@@ -340,6 +336,39 @@
 			#interrupt-cells = <3>;
 			#gpio-cells = <3>;
 
+			emac_rgmii_pins: emac-rgmii-pins {
+				pins = "PD2", "PD3", "PD4", "PD5", "PD6", "PD7",
+				       "PD11", "PD12", "PD13", "PD14", "PD18",
+				       "PD19", "PD21", "PD22", "PD23";
+				function = "gmac";
+				/*
+				 * data lines in RGMII mode use DDR mode
+				 * and need a higher signal drive strength
+				 */
+				drive-strength = <40>;
+			};
+
+			i2c0_pins: i2c0-pins {
+				pins = "PH0", "PH1";
+				function = "i2c0";
+			};
+
+			i2c1_pins: i2c1-pins {
+				pins = "PH2", "PH3";
+				function = "i2c1";
+			};
+
+			i2c2_ph_pins: i2c2-ph-pins {
+				pins = "PH4", "PH5";
+				function = "i2c2";
+			};
+
+			i2s1_pins: i2s1-pins {
+				/* I2S1 does not have external MCLK pin */
+				pins = "PG10", "PG11", "PG12", "PG13";
+				function = "i2s1";
+			};
+
 			mmc0_pins: mmc0-pins {
 				pins = "PF0", "PF1", "PF2",
 				       "PF3", "PF4", "PF5";
@@ -348,6 +377,14 @@
 				bias-pull-up;
 			};
 
+			mmc1_pins: mmc1-pins {
+				pins = "PG0", "PG1", "PG2",
+				       "PG3", "PG4", "PG5";
+				function = "mmc1";
+				drive-strength = <30>;
+				bias-pull-up;
+			};
+
 			mmc2_8bit_emmc_pins: mmc2-8bit-emmc-pins {
 				pins = "PC5", "PC6", "PC8", "PC9",
 				       "PC10", "PC11", "PC12", "PC13",
@@ -371,6 +408,16 @@
 				pins = "PF2", "PF4";
 				function = "uart0";
 			};
+
+			uart1_pins: uart1-pins {
+				pins = "PG6", "PG7";
+				function = "uart1";
+			};
+
+			uart1_rts_cts_pins: uart1-rts-cts-pins {
+				pins = "PG8", "PG9";
+				function = "uart1";
+			};
 		};
 
 		timer@1c20c00 {
@@ -404,7 +451,48 @@
 			status = "disabled";
 		};
 
-		uart0: serial@01c28000 {
+		i2s0: i2s@1c22000 {
+			#sound-dai-cells = <0>;
+			compatible = "allwinner,sun8i-a83t-i2s";
+			reg = <0x01c22000 0x400>;
+			interrupts = <GIC_SPI 13 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2S0>, <&ccu CLK_I2S0>;
+			clock-names = "apb", "mod";
+			dmas = <&dma 3>, <&dma 3>;
+			resets = <&ccu RST_BUS_I2S0>;
+			dma-names = "rx", "tx";
+			status = "disabled";
+		};
+
+		i2s1: i2s@1c22400 {
+			#sound-dai-cells = <0>;
+			compatible = "allwinner,sun8i-a83t-i2s";
+			reg = <0x01c22400 0x400>;
+			interrupts = <GIC_SPI 14 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2S1>, <&ccu CLK_I2S1>;
+			clock-names = "apb", "mod";
+			dmas = <&dma 4>, <&dma 4>;
+			resets = <&ccu RST_BUS_I2S1>;
+			dma-names = "rx", "tx";
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2s1_pins>;
+			status = "disabled";
+		};
+
+		i2s2: i2s@1c22800 {
+			#sound-dai-cells = <0>;
+			compatible = "allwinner,sun8i-a83t-i2s";
+			reg = <0x01c22800 0x400>;
+			interrupts = <GIC_SPI 99 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2S2>, <&ccu CLK_I2S2>;
+			clock-names = "apb", "mod";
+			dmas = <&dma 27>;
+			resets = <&ccu RST_BUS_I2S2>;
+			dma-names = "tx";
+			status = "disabled";
+		};
+
+		uart0: serial@1c28000 {
 			compatible = "snps,dw-apb-uart";
 			reg = <0x01c28000 0x400>;
 			interrupts = <GIC_SPI 0 IRQ_TYPE_LEVEL_HIGH>;
@@ -415,6 +503,78 @@
 			status = "disabled";
 		};
 
+		i2c0: i2c@1c2ac00 {
+			compatible = "allwinner,sun8i-a83t-i2c",
+				     "allwinner,sun6i-a31-i2c";
+			reg = <0x01c2ac00 0x400>;
+			interrupts = <GIC_SPI 6 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2C0>;
+			resets = <&ccu RST_BUS_I2C0>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c0_pins>;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		i2c1: i2c@1c2b000 {
+			compatible = "allwinner,sun8i-a83t-i2c",
+				     "allwinner,sun6i-a31-i2c";
+			reg = <0x01c2b000 0x400>;
+			interrupts = <GIC_SPI 7 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2C1>;
+			resets = <&ccu RST_BUS_I2C1>;
+			pinctrl-names = "default";
+			pinctrl-0 = <&i2c1_pins>;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		i2c2: i2c@1c2b400 {
+			compatible = "allwinner,sun8i-a83t-i2c",
+				     "allwinner,sun6i-a31-i2c";
+			reg = <0x01c2b400 0x400>;
+			interrupts = <GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2C2>;
+			resets = <&ccu RST_BUS_I2C2>;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		emac: ethernet@1c30000 {
+			compatible = "allwinner,sun8i-a83t-emac";
+			syscon = <&syscon>;
+			reg = <0x01c30000 0x104>;
+			interrupts = <GIC_SPI 82 IRQ_TYPE_LEVEL_HIGH>;
+			interrupt-names = "macirq";
+			resets = <&ccu 13>;
+			reset-names = "stmmaceth";
+			clocks = <&ccu 27>;
+			clock-names = "stmmaceth";
+			#address-cells = <1>;
+			#size-cells = <0>;
+			status = "disabled";
+
+			mdio: mdio {
+				compatible = "snps,dwmac-mdio";
+				#address-cells = <1>;
+				#size-cells = <0>;
+			};
+		};
+
+		uart1: serial@1c28400 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x01c28400 0x400>;
+			interrupts = <GIC_SPI 1 IRQ_TYPE_LEVEL_HIGH>;
+			reg-shift = <2>;
+			reg-io-width = <4>;
+			clocks = <&ccu CLK_BUS_UART1>;
+			resets = <&ccu RST_BUS_UART1>;
+			status = "disabled";
+		};
+
 		gic: interrupt-controller@1c81000 {
 			compatible = "arm,cortex-a7-gic", "arm,cortex-a15-gic";
 			reg = <0x01c81000 0x1000>,
diff --git a/arch/arm/boot/dts/sun8i-r40-bananapi-m2-ultra.dts b/arch/arm/boot/dts/sun8i-r40-bananapi-m2-ultra.dts
new file mode 100644
index 0000000..5587d72
--- /dev/null
+++ b/arch/arm/boot/dts/sun8i-r40-bananapi-m2-ultra.dts
@@ -0,0 +1,228 @@
+/*
+ * Copyright (C) 2017 Chen-Yu Tsai <wens@csie.org>
+ * Copyright (C) 2017 Icenowy Zheng <icenowy@aosc.io>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This file is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+/dts-v1/;
+#include "sun8i-r40.dtsi"
+
+#include <dt-bindings/gpio/gpio.h>
+
+/ {
+	model = "Banana Pi BPI-M2-Ultra";
+	compatible = "sinovoip,bpi-m2-ultra", "allwinner,sun8i-r40";
+
+	aliases {
+		serial0 = &uart0;
+	};
+
+	chosen {
+		stdout-path = "serial0:115200n8";
+	};
+
+	leds {
+		compatible = "gpio-leds";
+
+		pwr-led {
+			label = "bananapi:red:pwr";
+			gpios = <&pio 7 20 GPIO_ACTIVE_HIGH>;
+			default-state = "on";
+		};
+
+		user-led-green {
+			label = "bananapi:green:user";
+			gpios = <&pio 7 21 GPIO_ACTIVE_HIGH>;
+		};
+
+		user-led-blue {
+			label = "bananapi:blue:user";
+			gpios = <&pio 7 22 GPIO_ACTIVE_HIGH>;
+		};
+	};
+
+	reg_vcc5v0: vcc5v0 {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc5v0";
+		regulator-min-microvolt = <5000000>;
+		regulator-max-microvolt = <5000000>;
+		gpio = <&pio 7 23 GPIO_ACTIVE_HIGH>; /* PH23 */
+		enable-active-high;
+	};
+
+	wifi_pwrseq: wifi_pwrseq {
+		compatible = "mmc-pwrseq-simple";
+		reset-gpios = <&pio 6 10 GPIO_ACTIVE_LOW>; /* PG10 WIFI_EN */
+	};
+};
+
+&ehci1 {
+	status = "okay";
+};
+
+&ehci2 {
+	status = "okay";
+};
+
+&i2c0 {
+	status = "okay";
+
+	axp22x: pmic@34 {
+		compatible = "x-powers,axp221";
+		reg = <0x34>;
+		interrupt-parent = <&nmi_intc>;
+		interrupts = <0 IRQ_TYPE_LEVEL_LOW>;
+	};
+};
+
+#include "axp22x.dtsi"
+
+&ahci {
+	vdd1v2-supply = <&reg_eldo3>;
+	vdd2v5-supply = <&reg_dldo4>;
+	status = "okay";
+};
+
+&reg_aldo3 {
+	regulator-always-on;
+	regulator-min-microvolt = <2700000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "avcc";
+};
+
+&reg_dldo4 {
+	regulator-min-microvolt = <2500000>;
+	regulator-max-microvolt = <2500000>;
+	regulator-name = "vdd-2v5-sata";
+};
+
+&reg_eldo3 {
+	regulator-min-microvolt = <1200000>;
+	regulator-max-microvolt = <1200000>;
+	regulator-name = "vdd-1v2-sata";
+};
+
+&reg_dcdc1 {
+	regulator-always-on;
+	regulator-min-microvolt = <3000000>;
+	regulator-max-microvolt = <3000000>;
+	regulator-name = "vcc-3v0";
+};
+
+&reg_dcdc2 {
+	regulator-always-on;
+	regulator-min-microvolt = <1000000>;
+	regulator-max-microvolt = <1300000>;
+	regulator-name = "vdd-cpu";
+};
+
+&reg_dcdc3 {
+	regulator-always-on;
+	regulator-min-microvolt = <1000000>;
+	regulator-max-microvolt = <1300000>;
+	regulator-name = "vdd-sys";
+};
+
+&reg_dcdc5 {
+	regulator-always-on;
+	regulator-min-microvolt = <1500000>;
+	regulator-max-microvolt = <1500000>;
+	regulator-name = "vcc-dram";
+};
+
+&reg_dldo1 {
+	regulator-min-microvolt = <1800000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "vcc-wifi-io";
+};
+
+&reg_dldo2 {
+	regulator-min-microvolt = <3300000>;
+	regulator-max-microvolt = <3300000>;
+	regulator-name = "vcc-wifi";
+};
+
+&mmc0 {
+	vmmc-supply = <&reg_dcdc1>;
+	bus-width = <4>;
+	cd-gpios = <&pio 7 13 GPIO_ACTIVE_HIGH>; /* PH13 */
+	cd-inverted;
+	status = "okay";
+};
+
+&mmc1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc1_pg_pins>;
+	vmmc-supply = <&reg_dldo2>;
+	vqmmc-supply = <&reg_dldo1>;
+	mmc-pwrseq = <&wifi_pwrseq>;
+	bus-width = <4>;
+	non-removable;
+	status = "okay";
+};
+
+&mmc2 {
+	vmmc-supply = <&reg_dcdc1>;
+	vqmmc-supply = <&reg_dcdc1>;
+	bus-width = <8>;
+	non-removable;
+	status = "okay";
+};
+
+&ohci1 {
+	status = "okay";
+};
+
+&ohci2 {
+	status = "okay";
+};
+
+&uart0 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&uart0_pb_pins>;
+	status = "okay";
+};
+
+&usbphy {
+	usb1_vbus-supply = <&reg_vcc5v0>;
+	usb2_vbus-supply = <&reg_vcc5v0>;
+	pinctrl-names = "default";
+	status = "okay";
+};
diff --git a/arch/arm/boot/dts/sun8i-r40.dtsi b/arch/arm/boot/dts/sun8i-r40.dtsi
new file mode 100755
index 0000000..ef4df3b
--- /dev/null
+++ b/arch/arm/boot/dts/sun8i-r40.dtsi
@@ -0,0 +1,482 @@
+/*
+ * Copyright 2017 Chen-Yu Tsai <wens@csie.org>
+ * Copyright 2017 Icenowy Zheng <icenowy@aosc.io>
+ *
+ * This file is dual-licensed: you can use it either under the terms
+ * of the GPL or the X11 license, at your option. Note that this dual
+ * licensing only applies to this file, and not this project as a
+ * whole.
+ *
+ *  a) This file is free software; you can redistribute it and/or
+ *     modify it under the terms of the GNU General Public License as
+ *     published by the Free Software Foundation; either version 2 of the
+ *     License, or (at your option) any later version.
+ *
+ *     This file is distributed in the hope that it will be useful,
+ *     but WITHOUT ANY WARRANTY; without even the implied warranty of
+ *     MERCHANTABILITY or FITNESS FOR A PARTICULAR PURPOSE.  See the
+ *     GNU General Public License for more details.
+ *
+ * Or, alternatively,
+ *
+ *  b) Permission is hereby granted, free of charge, to any person
+ *     obtaining a copy of this software and associated documentation
+ *     files (the "Software"), to deal in the Software without
+ *     restriction, including without limitation the rights to use,
+ *     copy, modify, merge, publish, distribute, sublicense, and/or
+ *     sell copies of the Software, and to permit persons to whom the
+ *     Software is furnished to do so, subject to the following
+ *     conditions:
+ *
+ *     The above copyright notice and this permission notice shall be
+ *     included in all copies or substantial portions of the Software.
+ *
+ *     THE SOFTWARE IS PROVIDED "AS IS", WITHOUT WARRANTY OF ANY KIND,
+ *     EXPRESS OR IMPLIED, INCLUDING BUT NOT LIMITED TO THE WARRANTIES
+ *     OF MERCHANTABILITY, FITNESS FOR A PARTICULAR PURPOSE AND
+ *     NONINFRINGEMENT. IN NO EVENT SHALL THE AUTHORS OR COPYRIGHT
+ *     HOLDERS BE LIABLE FOR ANY CLAIM, DAMAGES OR OTHER LIABILITY,
+ *     WHETHER IN AN ACTION OF CONTRACT, TORT OR OTHERWISE, ARISING
+ *     FROM, OUT OF OR IN CONNECTION WITH THE SOFTWARE OR THE USE OR
+ *     OTHER DEALINGS IN THE SOFTWARE.
+ */
+
+#include <dt-bindings/interrupt-controller/arm-gic.h>
+#include <dt-bindings/clock/sun8i-r40-ccu.h>
+#include <dt-bindings/reset/sun8i-r40-ccu.h>
+
+/ {
+	#address-cells = <1>;
+	#size-cells = <1>;
+	interrupt-parent = <&gic>;
+
+	clocks {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		ranges;
+
+		osc24M: osc24M {
+			#clock-cells = <0>;
+			compatible = "fixed-clock";
+			clock-frequency = <24000000>;
+			clock-output-names = "osc24M";
+		};
+
+		osc32k: osc32k {
+			#clock-cells = <0>;
+			compatible = "fixed-clock";
+			clock-frequency = <32768>;
+			clock-output-names = "osc32k";
+		};
+	};
+
+	cpus {
+		#address-cells = <1>;
+		#size-cells = <0>;
+
+		cpu@0 {
+			compatible = "arm,cortex-a7";
+			device_type = "cpu";
+			reg = <0>;
+		};
+
+		cpu@1 {
+			compatible = "arm,cortex-a7";
+			device_type = "cpu";
+			reg = <1>;
+		};
+
+		cpu@2 {
+			compatible = "arm,cortex-a7";
+			device_type = "cpu";
+			reg = <2>;
+		};
+
+		cpu@3 {
+			compatible = "arm,cortex-a7";
+			device_type = "cpu";
+			reg = <3>;
+		};
+	};
+
+	soc {
+		compatible = "simple-bus";
+		#address-cells = <1>;
+		#size-cells = <1>;
+		ranges;
+
+		nmi_intc: interrupt-controller@1c00030 {
+			compatible = "allwinner,sun7i-a20-sc-nmi";
+			interrupt-controller;
+			#interrupt-cells = <2>;
+			reg = <0x01c00030 0x0c>;
+			interrupts = <GIC_SPI 0 IRQ_TYPE_LEVEL_HIGH>;
+		};
+
+		mmc0: mmc@1c0f000 {
+			compatible = "allwinner,sun8i-r40-mmc",
+				     "allwinner,sun50i-a64-mmc";
+			reg = <0x01c0f000 0x1000>;
+			clocks = <&ccu CLK_BUS_MMC0>, <&ccu CLK_MMC0>;
+			clock-names = "ahb", "mmc";
+			resets = <&ccu RST_BUS_MMC0>;
+			reset-names = "ahb";
+			pinctrl-0 = <&mmc0_pins>;
+			pinctrl-names = "default";
+			interrupts = <GIC_SPI 32 IRQ_TYPE_LEVEL_HIGH>;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		mmc1: mmc@1c10000 {
+			compatible = "allwinner,sun8i-r40-mmc",
+				     "allwinner,sun50i-a64-mmc";
+			reg = <0x01c10000 0x1000>;
+			clocks = <&ccu CLK_BUS_MMC1>, <&ccu CLK_MMC1>;
+			clock-names = "ahb", "mmc";
+			resets = <&ccu RST_BUS_MMC1>;
+			reset-names = "ahb";
+			interrupts = <GIC_SPI 33 IRQ_TYPE_LEVEL_HIGH>;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		mmc2: mmc@1c11000 {
+			compatible = "allwinner,sun8i-r40-emmc",
+				     "allwinner,sun50i-a64-emmc";
+			reg = <0x01c11000 0x1000>;
+			clocks = <&ccu CLK_BUS_MMC2>, <&ccu CLK_MMC2>;
+			clock-names = "ahb", "mmc";
+			resets = <&ccu RST_BUS_MMC2>;
+			reset-names = "ahb";
+			pinctrl-0 = <&mmc2_pins>;
+			pinctrl-names = "default";
+			interrupts = <GIC_SPI 34 IRQ_TYPE_LEVEL_HIGH>;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		mmc3: mmc@1c12000 {
+			compatible = "allwinner,sun8i-r40-mmc",
+				     "allwinner,sun50i-a64-mmc";
+			reg = <0x01c12000 0x1000>;
+			clocks = <&ccu CLK_BUS_MMC3>, <&ccu CLK_MMC3>;
+			clock-names = "ahb", "mmc";
+			resets = <&ccu RST_BUS_MMC3>;
+			reset-names = "ahb";
+			interrupts = <GIC_SPI 35 IRQ_TYPE_LEVEL_HIGH>;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		usbphy: phy@1c13400 {
+			compatible = "allwinner,sun8i-r40-usb-phy";
+			reg = <0x01c13400 0x14>,
+			      <0x01c14800 0x4>,
+			      <0x01c19800 0x4>,
+			      <0x01c1c800 0x4>;
+			reg-names = "phy_ctrl",
+				    "pmu0",
+				    "pmu1",
+				    "pmu2";
+			clocks = <&ccu CLK_USB_PHY0>,
+				 <&ccu CLK_USB_PHY1>,
+				 <&ccu CLK_USB_PHY2>;
+			clock-names = "usb0_phy",
+				      "usb1_phy",
+				      "usb2_phy";
+			resets = <&ccu RST_USB_PHY0>,
+				 <&ccu RST_USB_PHY1>,
+				 <&ccu RST_USB_PHY2>;
+			reset-names = "usb0_reset",
+				      "usb1_reset",
+				      "usb2_reset";
+			status = "disabled";
+			#phy-cells = <1>;
+		};
+
+		ehci1: usb@1c19000 {
+			compatible = "allwinner,sun8i-r40-ehci", "generic-ehci";
+			reg = <0x01c19000 0x100>;
+			interrupts = <GIC_SPI 76 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_EHCI1>;
+			resets = <&ccu RST_BUS_EHCI1>;
+			phys = <&usbphy 1>;
+			phy-names = "usb";
+			status = "okay";
+		};
+
+		ohci1: usb@1c19400 {
+			compatible = "allwinner,sun8i-r40-ohci", "generic-ohci";
+			reg = <0x01c19400 0x100>;
+			interrupts = <GIC_SPI 64 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_OHCI1>,
+				 <&ccu CLK_USB_OHCI1>;
+			resets = <&ccu RST_BUS_OHCI1>;
+			phys = <&usbphy 1>;
+			phy-names = "usb";
+			status = "disabled";
+		};
+
+		ehci2: usb@1c1c000 {
+			compatible = "allwinner,sun8i-r40-ehci", "generic-ehci";
+			reg = <0x01c1c000 0x100>;
+			interrupts = <GIC_SPI 78 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_EHCI2>;
+			resets = <&ccu RST_BUS_EHCI2>;
+			phys = <&usbphy 2>;
+			phy-names = "usb";
+			status = "okay";
+		};
+
+		ohci2: usb@1c1c400 {
+			compatible = "allwinner,sun8i-r40-ohci", "generic-ohci";
+			reg = <0x01c1c400 0x100>;
+			interrupts = <GIC_SPI 65 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_OHCI2>,
+				 <&ccu CLK_USB_OHCI2>;
+			resets = <&ccu RST_BUS_OHCI2>;
+			phys = <&usbphy 2>;
+			phy-names = "usb";
+			status = "disabled";
+		};
+
+		ahci: sata@1c18000 {
+			compatible = "allwinner,sun8i-r40-ahci", "allwinner,sun4i-a10-ahci";
+			reg = <0x01c18000 0x1000>;
+			interrupts = <GIC_SPI 56 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_SATA>, <&ccu CLK_BUS_SATA>;
+			resets = <&ccu RST_BUS_SATA>;
+			status = "enabled";
+		};
+
+		ccu: clock@1c20000 {
+			compatible = "allwinner,sun8i-r40-ccu";
+			reg = <0x01c20000 0x400>;
+			clocks = <&osc24M>, <&osc32k>;
+			clock-names = "hosc", "losc";
+			#clock-cells = <1>;
+			#reset-cells = <1>;
+		};
+
+		pio: pinctrl@1c20800 {
+			compatible = "allwinner,sun8i-r40-pinctrl";
+			reg = <0x01c20800 0x400>;
+			interrupts = <GIC_SPI 28 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_PIO>, <&osc24M>, <&osc32k>;
+			clock-names = "apb", "hosc", "losc";
+			gpio-controller;
+			interrupt-controller;
+			#interrupt-cells = <3>;
+			#gpio-cells = <3>;
+
+			i2c0_pins: i2c0-pins {
+				pins = "PB0", "PB1";
+				function = "i2c0";
+			};
+
+			mmc0_pins: mmc0-pins {
+				pins = "PF0", "PF1", "PF2",
+				       "PF3", "PF4", "PF5";
+				function = "mmc0";
+				drive-strength = <30>;
+				bias-pull-up;
+			};
+
+			mmc1_pg_pins: mmc1-pg-pins {
+				pins = "PG0", "PG1", "PG2",
+				       "PG3", "PG4", "PG5";
+				function = "mmc1";
+				drive-strength = <30>;
+				bias-pull-up;
+			};
+
+			mmc2_pins: mmc2-pins {
+				pins = "PC5", "PC6", "PC7", "PC8", "PC9",
+				       "PC10", "PC11", "PC12", "PC13", "PC14",
+				       "PC15", "PC24";
+				function = "mmc2";
+				drive-strength = <30>;
+				bias-pull-up;
+			};
+
+			uart0_pb_pins: uart0-pb-pins {
+				pins = "PB22", "PB23";
+				function = "uart0";
+			};
+		};
+
+		wdt: watchdog@1c20c90 {
+			compatible = "allwinner,sun4i-a10-wdt";
+			reg = <0x01c20c90 0x10>;
+		};
+
+		uart0: serial@1c28000 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x01c28000 0x400>;
+			interrupts = <GIC_SPI 1 IRQ_TYPE_LEVEL_HIGH>;
+			reg-shift = <2>;
+			reg-io-width = <4>;
+			clocks = <&ccu CLK_BUS_UART0>;
+			resets = <&ccu RST_BUS_UART0>;
+			status = "disabled";
+		};
+
+		uart1: serial@1c28400 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x01c28400 0x400>;
+			interrupts = <GIC_SPI 2 IRQ_TYPE_LEVEL_HIGH>;
+			reg-shift = <2>;
+			reg-io-width = <4>;
+			clocks = <&ccu CLK_BUS_UART1>;
+			resets = <&ccu RST_BUS_UART1>;
+			status = "disabled";
+		};
+
+		uart2: serial@1c28800 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x01c28800 0x400>;
+			interrupts = <GIC_SPI 3 IRQ_TYPE_LEVEL_HIGH>;
+			reg-shift = <2>;
+			reg-io-width = <4>;
+			clocks = <&ccu CLK_BUS_UART2>;
+			resets = <&ccu RST_BUS_UART2>;
+			status = "disabled";
+		};
+
+		uart3: serial@1c28c00 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x01c28c00 0x400>;
+			interrupts = <GIC_SPI 4 IRQ_TYPE_LEVEL_HIGH>;
+			reg-shift = <2>;
+			reg-io-width = <4>;
+			clocks = <&ccu CLK_BUS_UART3>;
+			resets = <&ccu RST_BUS_UART3>;
+			status = "disabled";
+		};
+
+		uart4: serial@1c29000 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x01c29000 0x400>;
+			interrupts = <GIC_SPI 17 IRQ_TYPE_LEVEL_HIGH>;
+			reg-shift = <2>;
+			reg-io-width = <4>;
+			clocks = <&ccu CLK_BUS_UART4>;
+			resets = <&ccu RST_BUS_UART4>;
+			status = "disabled";
+		};
+
+		uart5: serial@1c29400 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x01c29400 0x400>;
+			interrupts = <GIC_SPI 18 IRQ_TYPE_LEVEL_HIGH>;
+			reg-shift = <2>;
+			reg-io-width = <4>;
+			clocks = <&ccu CLK_BUS_UART5>;
+			resets = <&ccu RST_BUS_UART5>;
+			status = "disabled";
+		};
+
+		uart6: serial@1c29800 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x01c29800 0x400>;
+			interrupts = <GIC_SPI 19 IRQ_TYPE_LEVEL_HIGH>;
+			reg-shift = <2>;
+			reg-io-width = <4>;
+			clocks = <&ccu CLK_BUS_UART6>;
+			resets = <&ccu RST_BUS_UART6>;
+			status = "disabled";
+		};
+
+		uart7: serial@1c29c00 {
+			compatible = "snps,dw-apb-uart";
+			reg = <0x01c29c00 0x400>;
+			interrupts = <GIC_SPI 20 IRQ_TYPE_LEVEL_HIGH>;
+			reg-shift = <2>;
+			reg-io-width = <4>;
+			clocks = <&ccu CLK_BUS_UART7>;
+			resets = <&ccu RST_BUS_UART7>;
+			status = "disabled";
+		};
+
+		i2c0: i2c@1c2ac00 {
+			compatible = "allwinner,sun6i-a31-i2c";
+			reg = <0x01c2ac00 0x400>;
+			interrupts = <GIC_SPI 7 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2C0>;
+			resets = <&ccu RST_BUS_I2C0>;
+			pinctrl-0 = <&i2c0_pins>;
+			pinctrl-names = "default";
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		i2c1: i2c@1c2b000 {
+			compatible = "allwinner,sun6i-a31-i2c";
+			reg = <0x01c2b000 0x400>;
+			interrupts = <GIC_SPI 8 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2C1>;
+			resets = <&ccu RST_BUS_I2C1>;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		i2c2: i2c@1c2b400 {
+			compatible = "allwinner,sun6i-a31-i2c";
+			reg = <0x01c2b400 0x400>;
+			interrupts = <GIC_SPI 9 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2C2>;
+			resets = <&ccu RST_BUS_I2C2>;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		i2c3: i2c@1c2b800 {
+			compatible = "allwinner,sun6i-a31-i2c";
+			reg = <0x01c2b800 0x400>;
+			interrupts = <GIC_SPI 88 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2C3>;
+			resets = <&ccu RST_BUS_I2C3>;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		i2c4: i2c@1c2c000 {
+			compatible = "allwinner,sun6i-a31-i2c";
+			reg = <0x01c2c000 0x400>;
+			interrupts = <GIC_SPI 89 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_I2C4>;
+			resets = <&ccu RST_BUS_I2C4>;
+			status = "disabled";
+			#address-cells = <1>;
+			#size-cells = <0>;
+		};
+
+		gic: interrupt-controller@1c81000 {
+			compatible = "arm,gic-400";
+			reg = <0x01c81000 0x1000>,
+			      <0x01c82000 0x1000>,
+			      <0x01c84000 0x2000>,
+			      <0x01c86000 0x2000>;
+			interrupt-controller;
+			#interrupt-cells = <3>;
+			interrupts = <GIC_PPI 9 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>;
+		};
+	};
+
+	timer {
+		compatible = "arm,armv7-timer";
+		interrupts = <GIC_PPI 13 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 14 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 11 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>,
+			     <GIC_PPI 10 (GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_LOW)>;
+	};
+};
diff --git a/drivers/phy/allwinner/phy-sun4i-usb.c b/drivers/phy/allwinner/phy-sun4i-usb.c
index 1161e11..9df7a2c 100644
--- a/drivers/phy/allwinner/phy-sun4i-usb.c
+++ b/drivers/phy/allwinner/phy-sun4i-usb.c
@@ -112,6 +112,7 @@ enum sun4i_usb_phy_type {
 	sun8i_a33_phy,
 	sun8i_a83t_phy,
 	sun8i_h3_phy,
+	sun8i_r40_phy,
 	sun8i_v3s_phy,
 	sun50i_a64_phy,
 };
@@ -919,6 +920,16 @@ static const struct sun4i_usb_phy_cfg sun8i_h3_cfg = {
 	.phy0_dual_route = true,
 };
 
+static const struct sun4i_usb_phy_cfg sun8i_r40_cfg = {
+	.num_phys = 3,
+	.type = sun8i_r40_phy,
+	.disc_thresh = 3,
+	.phyctl_offset = REG_PHYCTL_A33,
+	.dedicated_clocks = true,
+	.enable_pmu_unk1 = true,
+	.phy0_dual_route = true,
+};
+
 static const struct sun4i_usb_phy_cfg sun8i_v3s_cfg = {
 	.num_phys = 1,
 	.type = sun8i_v3s_phy,
@@ -947,6 +958,7 @@ static const struct of_device_id sun4i_usb_phy_of_match[] = {
 	{ .compatible = "allwinner,sun8i-a33-usb-phy", .data = &sun8i_a33_cfg },
 	{ .compatible = "allwinner,sun8i-a83t-usb-phy", .data = &sun8i_a83t_cfg },
 	{ .compatible = "allwinner,sun8i-h3-usb-phy", .data = &sun8i_h3_cfg },
+	{ .compatible = "allwinner,sun8i-r40-usb-phy", .data = &sun8i_r40_cfg },
 	{ .compatible = "allwinner,sun8i-v3s-usb-phy", .data = &sun8i_v3s_cfg },
 	{ .compatible = "allwinner,sun50i-a64-usb-phy",
 	  .data = &sun50i_a64_cfg},
diff --git a/sound/soc/sunxi/sun4i-i2s.c b/sound/soc/sunxi/sun4i-i2s.c
index 7826fb3..1a7fef8 100644
--- a/sound/soc/sunxi/sun4i-i2s.c
+++ b/sound/soc/sunxi/sun4i-i2s.c
@@ -905,6 +905,23 @@ static const struct sun4i_i2s_quirks sun6i_a31_i2s_quirks = {
 	.field_rxchansel	= REG_FIELD(SUN4I_I2S_RX_CHAN_SEL_REG, 0, 2),
 };
 
+static const struct sun4i_i2s_quirks sun8i_a83t_i2s_quirks = {
+	.has_reset		= true,
+	.reg_offset_txdata	= SUN8I_I2S_FIFO_TX_REG,
+	.sun4i_i2s_regmap	= &sun4i_i2s_regmap_config,
+	.field_clkdiv_mclk_en	= REG_FIELD(SUN4I_I2S_CLK_DIV_REG, 7, 7),
+	.field_fmt_wss		= REG_FIELD(SUN4I_I2S_FMT0_REG, 2, 3),
+	.field_fmt_sr		= REG_FIELD(SUN4I_I2S_FMT0_REG, 4, 5),
+	.field_fmt_bclk		= REG_FIELD(SUN4I_I2S_FMT0_REG, 6, 6),
+	.field_fmt_lrclk	= REG_FIELD(SUN4I_I2S_FMT0_REG, 7, 7),
+	.has_slave_select_bit	= true,
+	.field_fmt_mode		= REG_FIELD(SUN4I_I2S_FMT0_REG, 0, 1),
+	.field_txchanmap	= REG_FIELD(SUN4I_I2S_TX_CHAN_MAP_REG, 0, 31),
+	.field_rxchanmap	= REG_FIELD(SUN4I_I2S_RX_CHAN_MAP_REG, 0, 31),
+	.field_txchansel	= REG_FIELD(SUN4I_I2S_TX_CHAN_SEL_REG, 0, 2),
+	.field_rxchansel	= REG_FIELD(SUN4I_I2S_RX_CHAN_SEL_REG, 0, 2),
+};
+
 static const struct sun4i_i2s_quirks sun8i_h3_i2s_quirks = {
 	.has_reset		= true,
 	.reg_offset_txdata	= SUN8I_I2S_FIFO_TX_REG,
@@ -1136,6 +1153,10 @@ static const struct of_device_id sun4i_i2s_match[] = {
 		.data = &sun6i_a31_i2s_quirks,
 	},
 	{
+		.compatible = "allwinner,sun8i-a83t-i2s",
+		.data = &sun8i_a83t_i2s_quirks,
+	},
+	{
 		.compatible = "allwinner,sun8i-h3-i2s",
 		.data = &sun8i_h3_i2s_quirks,
 	},
