diff --git a/arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts b/arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts
index d756ff8..e0df87d
--- a/arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts
+++ b/arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts
@@ -43,7 +43,6 @@
 /dts-v1/;
 #include "sun8i-h3.dtsi"
 #include "sunxi-common-regulators.dtsi"
-
 #include <dt-bindings/gpio/gpio.h>
 #include <dt-bindings/input/input.h>
 
@@ -61,6 +60,17 @@
 		stdout-path = "serial0:115200n8";
 	};
 
+	connector {
+		compatible = "hdmi-connector";
+		type = "a";
+
+		port {
+			hdmi_con_in: endpoint {
+				remote-endpoint = <&hdmi_out_con>;
+			};
+		};
+	};
+
 	leds {
 		compatible = "gpio-leds";
 		pinctrl-names = "default";
@@ -178,6 +188,40 @@
 	status = "okay";
 };
 
+&codec {
+	allwinner,audio-routing =
+		"Line Out", "LINEOUT",
+		"MIC1", "Mic",
+		"Mic",  "MBIAS";
+	status = "okay";
+};
+
+&de {
+	status = "okay";
+};
+
+&hdmi {
+	status = "okay";
+};
+
+&hdmi_out {
+	hdmi_out_con: endpoint {
+		remote-endpoint = <&hdmi_con_in>;
+	};
+};
+
+&i2s2 {
+	status = "okay";
+};
+
+&mixer0 {
+	status = "okay";
+};
+
+&tcon0 {
+	status = "okay";
+};
+
 &ohci0 {
 	status = "okay";
 };
@@ -190,6 +234,10 @@
 	status = "okay";
 };
 
+&r_i2c {
+	status = "okay";
+};
+
 &r_pio {
 	pwr_led_bpi_m2p: led_pins@0 {
 		pins = "PL10";
