diff --git a/arch/arm/boot/dts/sun8i-h3-nanopi-m1.dts b/arch/arm/boot/dts/sun8i-h3-nanopi-m1.dts
index ec63d10..9dff001
--- a/arch/arm/boot/dts/sun8i-h3-nanopi-m1.dts
+++ b/arch/arm/boot/dts/sun8i-h3-nanopi-m1.dts
@@ -45,6 +45,66 @@
 / {
 	model = "FriendlyArm NanoPi M1";
 	compatible = "friendlyarm,nanopi-m1", "allwinner,sun8i-h3";
+
+	connector {
+		compatible = "hdmi-connector";
+		type = "a";
+
+		port {
+			hdmi_con_in: endpoint {
+				remote-endpoint = <&hdmi_out_con>;
+			};
+		};
+	};
+};
+
+&emac {
+	phy-handle = <&int_mii_phy>;
+	phy-mode = "mii";
+	allwinner,leds-active-low;
+	status = "okay";
+};
+
+&codec {
+	allwinner,audio-routing =
+		"Line Out", "LINEOUT",
+		"MIC1", "Mic",
+		"Mic",  "MBIAS";
+	status = "okay";
+};
+
+&de {
+	status = "okay";
+};
+
+&hdmi {
+	status = "okay";
+};
+
+&hdmi_out {
+	hdmi_out_con: endpoint {
+		remote-endpoint = <&hdmi_con_in>;
+	};
+};
+
+&i2s2 {
+	status = "okay";
+};
+
+&mixer0 {
+	status = "okay";
+};
+
+&sound_hdmi {
+	status = "okay";
+};
+
+&tcon0 {
+	status = "okay";
+};
+
+&ehci0 {
+	status = "okay";
 };
 
 &ehci1 {
@@ -55,6 +115,14 @@
 	status = "okay";
 };
 
+&ehci3 {
+	status = "okay";
+};
+
+&ohci0 {
+	status = "okay";
+};
+
 &ohci1 {
 	status = "okay";
 };
@@ -62,3 +130,11 @@
 &ohci2 {
 	status = "okay";
 };
+
+&ohci3 {
+	status = "okay";
+};
+
+&r_i2c {
+	status = "okay";
+};
\ No newline at end of file
