diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
index 02c0385f..db616e73 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64.dtsi
@@ -105,6 +110,7 @@
 
 	timer {
 		compatible = "arm,armv8-timer";
+		fsl,erratum-a008585;
 		interrupts = <GIC_PPI 13
 			(GIC_CPU_MASK_SIMPLE(4) | IRQ_TYPE_LEVEL_HIGH)>,
 			     <GIC_PPI 14
