diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus2.dts b/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus2.dts
index ba4d6b1..d71a8b8
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus2.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5-orangepi-zero-plus2.dts
@@ -43,15 +43,17 @@
 /dts-v1/;
 
 #include "sun50i-h5.dtsi"
-
 #include <dt-bindings/gpio/gpio.h>
+#include <dt-bindings/input/input.h>
+#include <dt-bindings/pinctrl/sun4i-a10.h>
 
 / {
-	model = "OrangePi Zero Plus2";
+	model = "Xunlong Orange Pi Zero Plus2";
 	compatible = "xunlong,orangepi-zero-plus2", "allwinner,sun50i-h5";
 
 	aliases {
 		serial0 = &uart0;
+		ethernet1 = &brcmf;
 	};
 
 	chosen {
@@ -65,11 +67,29 @@
 		regulator-max-microvolt = <3300000>;
 	};
 
-        wifi_pwrseq: wifi_pwrseq {
-                compatible = "mmc-pwrseq-simple";
-                reset-gpios = <&pio 0 9 GPIO_ACTIVE_LOW>; /* PA9 */
-                post-power-on-delay-ms = <50>;
-        };
+    wifi_pwrseq: wifi_pwrseq {
+        compatible = "mmc-pwrseq-simple";
+        reset-gpios = <&pio 0 9 GPIO_ACTIVE_LOW>; /* PA9 */
+        post-power-on-delay-ms = <50>;
+    };
+
+	reg_sy8113b: gpio-regulator {
+		compatible = "regulator-gpio";
+		regulator-name = "vdd-cpux";
+		regulator-type = "voltage";
+		regulator-boot-on;
+		regulator-always-on;
+		regulator-min-microvolt = <1100000>;
+		regulator-max-microvolt = <1300000>;
+		regulator-ramp-delay = <50>; /* 4ms */
+
+		gpios = <&r_pio 0 6 GPIO_ACTIVE_HIGH>; /* PL6 */
+		enable-active-high;
+		gpios-states = <0x1>;
+		states = <1100000 0x0
+			  1300000 0x1>;
+	};
+
 };
 
 &mmc0 {
@@ -112,6 +132,43 @@
 	status = "okay";
 };
 
+&cpu0 {
+	cpu-supply = <&reg_sy8113b>;
+};
+
+&de {
+	status = "okay";
+};
+
+&ehci0 {
+	status = "okay";
+};
+
+&ohci0 {
+	status = "okay";
+};
+
+&spi0 {
+	/* Disable SPI NOR by default: it optional on Orange Pi Zero boards */
+	status = "disabled";
+
+	flash@0 {
+		#address-cells = <1>;
+		#size-cells = <1>;
+		compatible = "mxicy,mx25l1606e", "winbond,w25q128";
+		reg = <0>;
+		spi-max-frequency = <40000000>;
+	};
+};
+
+&hdmi {
+	status = "okay";
+};
+
+&mixer0 {
+	status = "okay";
+};
+
 &r_pio {
 	wifi_wake: wifi_wake@0 {
 		pins = "PL7";
@@ -120,8 +177,35 @@
 	};
 };
 
+&sound_hdmi {
+	status = "okay";
+};
+
+&tcon0 {
+	status = "okay";
+};
+
+&r_i2c {
+	status = "okay";
+};
+
 &uart0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&uart0_pins_a>;
 	status = "okay";
 };
+
+&usb_otg {
+	dr_mode = "peripheral";
+	status = "okay";
+};
+
+&usbphy {
+	/*
+	 * USB Type-A port VBUS is always on. However, MicroUSB VBUS can only
+	 * power up the board; when it's used as OTG port, this VBUS is
+	 * always off even if the board is powered via GPIO pins.
+	 */
+	usb0_id_det-gpios = <&pio 6 12 GPIO_ACTIVE_HIGH>; /* PG12 */
+	status = "okay";
+};
\ No newline at end of file
