diff --git a/arch/arm/boot/dts/sunxi-h3-h5.dtsi b/arch/arm/boot/dts/sunxi-h3-h5.dtsi
index ccde3a00..44ae22a9 100644
--- a/arch/arm/boot/dts/sunxi-h3-h5.dtsi
+++ b/arch/arm/boot/dts/sunxi-h3-h5.dtsi
@@ -109,6 +109,42 @@
 			assigned-clock-rates = <432000000>;
 		};
 
+		hdmi: hdmi@1ee0000 {
+			compatible = "allwinner,sun8i-h3-dw-hdmi";
+			reg = <0x01ee0000 0x10000>,
+			      <0x01ef0000 0x10000>;
+			reg-io-width = <1>;
+			interrupts = <GIC_SPI 88 IRQ_TYPE_LEVEL_HIGH>;
+			clocks = <&ccu CLK_BUS_HDMI>, <&ccu CLK_HDMI>,
+				 <&ccu CLK_HDMI_DDC>;
+			clock-names = "iahb", "isfr", "ddc";
+			resets = <&ccu RST_BUS_HDMI0>, <&ccu RST_BUS_HDMI1>;
+			reset-names = "hdmi", "ddc";
+			status = "disabled";
+
+			ports {
+				#address-cells = <1>;
+				#size-cells = <0>;
+
+				hdmi_in: port@0 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <0>;
+
+					hdmi_in_tcon0: endpoint@0 {
+						reg = <0>;
+						remote-endpoint = <&tcon0_out_hdmi>;
+					};
+				};
+
+				hdmi_out: port@1 {
+					#address-cells = <1>;
+					#size-cells = <0>;
+					reg = <1>;
+				};
+			};
+		};
+
 		mixer0: mixer@1100000 {
 			compatible = "allwinner,sun8i-h3-de2-mixer0";
 			reg = <0x01100000 0x100000>;
@@ -224,6 +260,11 @@
 					#address-cells = <1>;
 					#size-cells = <0>;
 					reg = <1>;
+
+					tcon0_out_hdmi: endpoint@1 {
+						reg = <1>;
+						remote-endpoint = <&hdmi_in_tcon0>;
+					};
 				};
 			};
 		};
