From b804df86f96f4bdc74abab55404a0bdcc7526f8b Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Sun, 12 Nov 2017 06:25:17 +0100
Subject: [PATCH 46/82] ARM: dts: sun8i-a83t: Add lradc

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm/boot/dts/sun8i-a83t.dtsi | 7 +++++++
 1 file changed, 7 insertions(+)

diff --git a/arch/arm/boot/dts/sun8i-a83t.dtsi b/arch/arm/boot/dts/sun8i-a83t.dtsi
index 66f035ead79a..d9074f050a9c 100644
--- a/arch/arm/boot/dts/sun8i-a83t.dtsi
+++ b/arch/arm/boot/dts/sun8i-a83t.dtsi
@@ -627,6 +627,13 @@
 			status = "disabled";
 		};
 
+		lradc: lradc@1f03c00 {
+			compatible = "allwinner,sun4i-a10-lradc-keys";
+			reg = <0x01f03c00 0x100>;
+			interrupts = <GIC_SPI 42 IRQ_TYPE_LEVEL_HIGH>;
+			status = "disabled";
+		};
+
 		ccu: clock@1c20000 {
 			compatible = "allwinner,sun8i-a83t-ccu";
 			reg = <0x01c20000 0x400>;
-- 
2.20.1

