diff --git a/arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts b/arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts
index 195a75d..f3f324e 100644
--- a/arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts
+++ b/arch/arm/boot/dts/sun8i-h3-bananapi-m2-plus.dts
@@ -48,3 +48,8 @@
 	model = "Banana Pi BPI-M2-Plus H3";
 	compatible = "sinovoip,bpi-m2-plus", "allwinner,sun8i-h3";
 };
+
+&wifi_pwrseq {
+		clocks = <&rtc 1>;
+		clock-names = "ext_clock";
+};
