diff --git a/arch/arm/dts/sun50i-a64-orangepi-win.dts b/arch/arm/dts/sun50i-a64-orangepi-win.dts
index 2c39d10..819fd97
--- a/arch/arm/dts/sun50i-a64-orangepi-win.dts
+++ b/arch/arm/dts/sun50i-a64-orangepi-win.dts
@@ -151,6 +151,16 @@
 	};
 };
 
+&i2c1 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&i2c1_pins>;
+	status = "okay";
+};
+
+&i2c1_pins {
+	bias-pull-up;
+};
+
 &mmc0 {
 	pinctrl-names = "default";
 	pinctrl-0 = <&mmc0_pins>;
@@ -172,6 +182,16 @@
 	status = "okay";
 };
 
+&mmc2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc2_pins>;
+	vmmc-supply = <&reg_dcdc1>;
+	bus-width = <8>;
+	non-removable;
+	cap-mmc-hw-reset;
+ 	status = "okay";
+};
+
 &ohci0 {
 	status = "okay";
 };
diff --git a/configs/orangepi_win_defconfig b/configs/orangepi_win_defconfig
index ab889ea..6f16cc0 100644
--- a/configs/orangepi_win_defconfig
+++ b/configs/orangepi_win_defconfig
@@ -5,6 +5,8 @@ CONFIG_MACH_SUN50I=y
 CONFIG_RESERVE_ALLWINNER_BOOT0_HEADER=y
 CONFIG_SPL_SPI_SUNXI=y
 CONFIG_NR_DRAM_BANKS=1
+CONFIG_MMC0_CD_PIN="PH13"
+CONFIG_MMC_SUNXI_SLOT_EXTRA=2
 # CONFIG_SYS_MALLOC_CLEAR_ON_INIT is not set
 # CONFIG_CMD_FLASH is not set
 # CONFIG_SPL_DOS_PARTITION is not set
