diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
index fd6681ab9..89e0837d7 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h6.dtsi
@@ -216,6 +216,14 @@
 				bias-pull-up;
 			};
 
+			mmc1_pins: mmc1-pins {
+				pins = "PG0", "PG1", "PG2", "PG3",
+				       "PG4", "PG5";
+				function = "mmc1";
+				drive-strength = <30>;
+				bias-pull-up;
+			};
+
 			mmc2_pins: mmc2-pins {
 				pins = "PC1", "PC4", "PC5", "PC6",
 				       "PC7", "PC8", "PC9", "PC10",
