diff --git a/arch/arm/dts/sun50i-a64-olinuxino.dts b/arch/arm/dts/sun50i-a64-olinuxino.dts
index f7a4bcc..9d77afb 100644
--- a/arch/arm/dts/sun50i-a64-olinuxino.dts
+++ b/arch/arm/dts/sun50i-a64-olinuxino.dts
@@ -155,6 +155,16 @@
 	};
 };
 
+&mmc2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc2_pins>;
+	vmmc-supply = <&reg_dcdc1>;
+	bus-width = <8>;
+	non-removable;
+	cap-mmc-hw-reset;
+	status = "okay";
+};
+
 &ohci0 {
 	status = "okay";
 };
