diff --git a/arch/arm64/boot/dts/allwinner/sun50i-a64-olinuxino.dts b/arch/arm64/boot/dts/allwinner/sun50i-a64-olinuxino.dts
index 3b3081b..24cde3d 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-a64-olinuxino.dts
+++ b/arch/arm64/boot/dts/allwinner/sun50i-a64-olinuxino.dts
@@ -81,6 +81,13 @@
 		status = "okay";
 	};
 	
+	reg_vcc3v3: vcc3v3 {
+		compatible = "regulator-fixed";
+		regulator-name = "vcc3v3";
+		regulator-min-microvolt = <3300000>;
+		regulator-max-microvolt = <3300000>;
+	};
+	
 	wifi_pwrseq: wifi_pwrseq {
 		compatible = "mmc-pwrseq-simple";
 		reset-gpios = <&r_pio 0 2 GPIO_ACTIVE_LOW>; /* PL2 */
@@ -92,6 +99,16 @@
 	};
 };
 
+&mmc2 {
+	pinctrl-names = "default";
+	pinctrl-0 = <&mmc2_pins>;
+	vmmc-supply = <&reg_vcc3v3>;
+	bus-width = <8>;
+	non-removable;
+	cap-mmc-hw-reset;
+	status = "okay";
+};
+
 &r_rsb {
 	status = "okay";
 
