From d2deb88ff41a528b4c35f1f6e344e6a097eabedd Mon Sep 17 00:00:00 2001
From: Icenowy Zheng <icenowy@aosc.io>
Date: Tue, 4 Sep 2018 12:40:51 +0800
Subject: [PATCH 099/146] dt-bindings: sun4i-drm: add HDMI VCC supply property
 for sun8i-dw-hdmi

Allwiner SoCs with DesignWare HDMI controller all come with a "HVCC"
pin, which is the VCC of HDMI part.

Add a supply property to specify HVCC's regulator in the device tree.

Signed-off-by: Icenowy Zheng <icenowy@aosc.io>
---
 Documentation/devicetree/bindings/display/sunxi/sun4i-drm.txt | 3 +++
 1 file changed, 3 insertions(+)

diff --git a/Documentation/devicetree/bindings/display/sunxi/sun4i-drm.txt b/Documentation/devicetree/bindings/display/sunxi/sun4i-drm.txt
index fdb8fb29033f..0bbb5d47f228 100644
--- a/Documentation/devicetree/bindings/display/sunxi/sun4i-drm.txt
+++ b/Documentation/devicetree/bindings/display/sunxi/sun4i-drm.txt
@@ -97,6 +97,9 @@ Required properties:
     first port should be the input endpoint. The second should be the
     output, usually to an HDMI connector.
 
+Optional properties:
+  - hvcc-supply: the VCC power supply of the controller
+
 DWC HDMI PHY
 ------------
 
-- 
2.17.1

