From 6352f285dc5071be981ac30d72b4fbd11bed7fcd Mon Sep 17 00:00:00 2001
From: Ondrej Jirman <megous@megous.com>
Date: Sat, 30 Jun 2018 07:58:54 +0200
Subject: [PATCH 72/82] ARM: dts: sun8i-a83t: Add missing cooling-cells
 properties to cpu nodes

Signed-off-by: Ondrej Jirman <megous@megous.com>
---
 arch/arm/boot/dts/sun8i-a83t.dtsi | 10 ++++++----
 1 file changed, 6 insertions(+), 4 deletions(-)

diff --git a/arch/arm/boot/dts/sun8i-a83t.dtsi b/arch/arm/boot/dts/sun8i-a83t.dtsi
index 17371e0614e2..cb0607580d04 100644
--- a/arch/arm/boot/dts/sun8i-a83t.dtsi
+++ b/arch/arm/boot/dts/sun8i-a83t.dtsi
@@ -72,8 +72,6 @@
 			enable-method = "allwinner,sun8i-a83t-smp";
 			reg = <0>;
 			#cooling-cells = <2>;
-			cooling-min-level = <0>;
-			cooling-max-level = <7>;
 		};
 
 		cpu@1 {
@@ -86,6 +84,7 @@
 			cci-control-port = <&cci_control0>;
 			enable-method = "allwinner,sun8i-a83t-smp";
 			reg = <1>;
+			#cooling-cells = <2>;
 		};
 
 		cpu@2 {
@@ -98,6 +97,7 @@
 			cci-control-port = <&cci_control0>;
 			enable-method = "allwinner,sun8i-a83t-smp";
 			reg = <2>;
+			#cooling-cells = <2>;
 		};
 
 		cpu@3 {
@@ -110,6 +110,7 @@
 			cci-control-port = <&cci_control0>;
 			enable-method = "allwinner,sun8i-a83t-smp";
 			reg = <3>;
+			#cooling-cells = <2>;
 		};
 
 		cpu100: cpu@100 {
@@ -123,8 +124,6 @@
 			enable-method = "allwinner,sun8i-a83t-smp";
 			reg = <0x100>;
 			#cooling-cells = <2>;
-			cooling-min-level = <0>;
-			cooling-max-level = <7>;
 		};
 
 		cpu@101 {
@@ -137,6 +136,7 @@
 			cci-control-port = <&cci_control1>;
 			enable-method = "allwinner,sun8i-a83t-smp";
 			reg = <0x101>;
+			#cooling-cells = <2>;
 		};
 
 		cpu@102 {
@@ -149,6 +149,7 @@
 			cci-control-port = <&cci_control1>;
 			enable-method = "allwinner,sun8i-a83t-smp";
 			reg = <0x102>;
+			#cooling-cells = <2>;
 		};
 
 		cpu@103 {
@@ -161,6 +162,7 @@
 			cci-control-port = <&cci_control1>;
 			enable-method = "allwinner,sun8i-a83t-smp";
 			reg = <0x103>;
+			#cooling-cells = <2>;
 		};
 	};
 
-- 
2.20.1

