diff --git a/arch/arm/boot/dts/sun8i-h3.dtsi b/arch/arm/boot/dts/sun8i-h3.dtsi
index b36f9f42..b2896427 100644
--- a/arch/arm/boot/dts/sun8i-h3.dtsi
+++ b/arch/arm/boot/dts/sun8i-h3.dtsi
@@ -85,6 +85,14 @@
 	compatible = "allwinner,sun8i-h3-ccu";
 };
 
+&display_clocks {
+	compatible = "allwinner,sun8i-a83t-de2-clk";
+};
+
+&mixer1 {
+	resets = <&display_clocks RST_WB>;
+};
+
 &mmc0 {
 	compatible = "allwinner,sun7i-a20-mmc";
 	clocks = <&ccu CLK_BUS_MMC0>,
