From d2259cb25f16b469b558d3b8d652862a7c5ddef5 Mon Sep 17 00:00:00 2001
From: Icenowy Zheng <icenowy@aosc.io>
Date: Tue, 15 Aug 2017 21:35:39 +0800
Subject: [PATCH] arm64: allwinner: h5: support display pipelines

As we have extracted the display pipelines to the H3/H5 common DTSI, we
can now support the display pipelines on H5.

Signed-off-by: Icenowy Zheng <icenowy@aosc.io>
---
 arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi | 8 ++++++++
 1 file changed, 8 insertions(+)

diff --git a/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi b/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi
index d9a720bff05d3..305f7a28ba03c 100644
--- a/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi
+++ b/arch/arm64/boot/dts/allwinner/sun50i-h5.dtsi
@@ -98,6 +98,14 @@
 	compatible = "allwinner,sun50i-h5-ccu";
 };
 
+&display_clocks {
+	compatible = "allwinner,sun50i-h5-de2-clk";
+};
+
+&mixer1 {
+	resets = <&display_clocks RST_MIXER1>;
+};
+
 &mmc0 {
 	compatible = "allwinner,sun50i-h5-mmc",
 		     "allwinner,sun50i-a64-mmc";
